# ISO 19115-3 Codelist Report

## Codelists from the Metadata for Resource Content (mrc) Namespace

Scope | Codelists related to Metadata for Resource Content (mrc) Namespace
Field of Application | ISO TC211 Metadata Standards
Version (Date) | 1.0 ()

## MD_CoverageContentTypeCode ( MD_CoverageContentTypeCode ):

Description: specific type of information represented in the cell

Entry | Definition
--- | ---
MD_CoverageContentTypeCode_image | meaningful numerical representation of a physical parameter that is not the actual value of the physical parameter
MD_CoverageContentTypeCode_thematicClassification | code value with no quantitative meaning, used to represent a physical quantity
MD_CoverageContentTypeCode_physicalMeasurement | value in physical units of the quantity being measured
MD_CoverageContentTypeCode_auxillaryInformation | data, usually a physical measurement, used to support the calculation of the primary physicalMeasurement coverages in the dataset (e.g. grid of aerosol optical thickness used in the calculation of a sea surface temperature product).
MD_CoverageContentTypeCode_qualityInformation | data used to characterize the quality of the physicalMeasurement coverages in the dataset. Typically included in a gmi:QE_CoverageResult.
MD_CoverageContentTypeCode_referenceInformation | reference information used to support the calculation or use of the physicalMeasurement coverages in the dataset (e.g. grids of latitude/longitude used to geolocate the physical measurements).
MD_CoverageContentTypeCode_modelResult | resources with values that are calculated using a model rather than being observed or calculated from observations.
MD_CoverageContentTypeCode_coordinate | data used to provide coordinate axis values

top

## MD_ImagingConditionCode ( MD_ImagingConditionCode ):

Description: code which indicates conditions which may affect the image

Entry | Definition
--- | ---
MD_ImagingConditionCode_blurredImage | portion of the image is blurred
MD_ImagingConditionCode_cloud | portion of the image is partially obscured by cloud cover
MD_ImagingConditionCode_degradingObliquity | acute angle between the plane of the ecliptic (the plane of the Earth s orbit) and the plane of the celestial equator
MD_ImagingConditionCode_fog | portion of the image is partially obscured by fog
MD_ImagingConditionCode_heavySmokeOrDust | portion of the image is partially obscured by heavy smoke or dust
MD_ImagingConditionCode_night | image was taken at night
MD_ImagingConditionCode_rain | image was taken during rainfall
MD_ImagingConditionCode_semiDarkness | image was taken during semi-dark conditions; twilight conditions
MD_ImagingConditionCode_shadow | portion of the image is obscured by shadow
MD_ImagingConditionCode_snow | portion of the image is obscured by snow
MD_ImagingConditionCode_terrainMasking | the absence of collection data of a given point or area caused by the relative location of topographic features which obstruct the collection path between the collector(s) and the subject(s) of interest

top

Stylesheet: CT_CodelistHTML.xsl Version: 2015-04-17