# Feature type: Camp_S

## Package: Settlements
## Title: AI030_S
## Definition: An encampment where tents and/or other easily moveable structures (for example: yurts) serve as temporary residences.
## Description: A permanent camp would be classified as Built-Up Area.
## Type: Feature type
## Overview of characteristics:
Attributes and association roles
Name | Type | Multiplicity
--- | --- | ---
controllingAuthority | Camp_controllingAuthority | 0..1
facilityOperationalStatus | Camp_facilityOperationalStatus | 0..1
featureFunction | Camp_featureFunction | 0..1
featureFunction_2 | Camp_featureFunction | 0..1
featureFunction_3 | Camp_featureFunction | 0..1
geometry-surfaceGeometryInfo.baseElevation.accuracy | Real | 0..1
geometry-surfaceGeometryInfo.baseElevation.value-singleValue | Real | 0..1
geometry-surfaceGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.absoluteHorizAccEvalMeth | HorizPosAccuracy_absoluteHorizAccEvalMeth | 0..1
geometry-surfaceGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.value | Real | 0..1
geometry-surfaceGeometryInfo.horizCoordMetadata.horizAccuracyCategory | HorizCoordMetadata_horizAccuracyCategory | 0..1
geometry-surfaceGeometryInfo.surfaceGeometry | GM_Surface | 0..1
geometry-surfaceGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.absoluteVertAccEvalMeth | VertPosAccuracy_absoluteVertAccEvalMeth | 0..1
geometry-surfaceGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.value | Real | 0..1
geometry-surfaceGeometryInfo.vertCoordMetadata.elevationAccuracyCategory | VertCoordMetadata_elevationAccuracyCategory | 0..1
heightAboveSurfaceLevel.accuracy | Real | 0..1
heightAboveSurfaceLevel.value-singleValue | Real | 0..1
highestElevation.accuracy | Real | 0..1
highestElevation.value-singleValue | Real | 0..1
isDesignatedBy.fullName | CharacterString | 0..1
isDesignatedBy.fullNameNoDiacritics | CharacterString | 0..1
isDesignatedBy.fullNameOrdered | CharacterString | 0..1
isDesignatedBy.geoNameCharacterSet | GeoNameInfo_geoNameCharacterSet | 0..1
isDesignatedBy.geoNameDesignation | CharacterString | 0..1
isDesignatedBy.geographicNameType | GeoNameInfo_geographicNameType | 0..1
isDesignatedBy.iso15924ScriptCode | CharacterString | 0..1
isDesignatedBy.languageCode | CharacterString | 0..1
isDesignatedBy.languageDialectCode | CharacterString | 0..1
isDesignatedBy.multipleOfficialNames | BooleanWithONINA | 0..1
isDesignatedBy.nameIdentifier | CharacterString | 0..1
isDesignatedBy.namedFeatureIdentifier | CharacterString | 0..1
isDesignatedBy_2.fullName | CharacterString | 0..1
isDesignatedBy_2.fullNameNoDiacritics | CharacterString | 0..1
isDesignatedBy_2.fullNameOrdered | CharacterString | 0..1
isDesignatedBy_2.geoNameCharacterSet | GeoNameInfo_geoNameCharacterSet | 0..1
isDesignatedBy_2.geoNameDesignation | CharacterString | 0..1
isDesignatedBy_2.geographicNameType | GeoNameInfo_geographicNameType | 0..1
isDesignatedBy_2.iso15924ScriptCode | CharacterString | 0..1
isDesignatedBy_2.languageCode | CharacterString | 0..1
isDesignatedBy_2.languageDialectCode | CharacterString | 0..1
isDesignatedBy_2.multipleOfficialNames | BooleanWithONINA | 0..1
isDesignatedBy_2.nameIdentifier | CharacterString | 0..1
isDesignatedBy_2.namedFeatureIdentifier | CharacterString | 0..1
metadata.dataQualityStatement | CharacterString | 0..1
metadata.delineationKnown | BooleanWithONINA | 0..1
metadata.existenceCertaintyCat | FeatureMetadata_existenceCertaintyCat | 0..1
metadata.surveyCoverageCategory | FeatureMetadata_surveyCoverageCategory | 0..1
nomadicSeasonalLocation | Camp_nomadicSeasonalLocation | 0..1
nomadicSeasonalLocation_2 | Camp_nomadicSeasonalLocation | 0..1
nomadicSeasonalLocation_3 | Camp_nomadicSeasonalLocation | 0..1
physicalCondition | Camp_physicalCondition | 0..1
predominantFeatureHeight-singleValue | Real | 0..1
settlementPattern | Camp_settlementPattern | 0..1
specifiedDomainValues | CharacterString | 0..1
structMatType | Camp_structMatType | 0..1
structMatType_2 | Camp_structMatType | 0..1
structMatType_3 | Camp_structMatType | 0..1
structureDensity-singleValue | Real | 0..1
uniqueEntityIdentifier | CharacterString | 1
universalUniqueIdentifier | CharacterString | 1
## Attribute: back to top
Name: | controllingAuthority
Title: | CAA
Definition: | The controlling authority responsible for a facility or site.
Description: | Controlling authorities may be distinguished by organizational level (for example: national, sub-national, or military district) and/or type (for example: private or public).
Multiplicity: | 0..1
Value type: | Camp_controllingAuthority (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
private | 3 Administered by an individual or corporation, rather than a State or a public body.
military | 5 An armed force constituted under the laws of a State.
jointMilitaryCivilian | 7 An administrative body composed of both military and civil authorities. Often created during times of civil unrest or war and intended to be of a temporary nature.
civilian | 16 An administrative unit not associated with an armed force.
public | 17 Administered on behalf all members of a community, rather than restricted to an individual or corporation.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | facilityOperationalStatus
Title: | COS
Definition: | The status of operation of a man-made structure, as a whole.
Description: | Includes actual operations, operational capability, and planned or proposed man-made structures.
Multiplicity: | 0..1
Value type: | Camp_facilityOperationalStatus (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
planned | 6 Future operations are scheduled.
temporarilyNonOperational | 9 Temporarily not in operation due to it being non-functional and operation is scheduled to be restored. Usually an unscheduled loss of operation.
operational | 13 Fully capable of operation. The schedule of operations may be indeterminate or unknown.
notInOperation | 8 Fully functional and ready for operation however has not been certified or commissioned for such use. The operational capacity may not be authorized for various reasons, such as newly installed and not yet commissioned or certified, or operational but has been taken out of service for non-technical reasons, awaiting certification or commissioning status.
partiallyOperational | 14 Functional, but operating with only partial capability for some reason. Parts of the man-made structure are not in operation; or, the operation is running below capacity.
nonOperational | 4 Not in operation due to it being non-functional and operation is not scheduled to be restored.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | featureFunction
Title: | FFN
Definition: | The purpose(s) of, or intended role(s) served by, the feature.
Multiplicity: | 0..1
Value type: | Camp_featureFunction (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
migrantLabour | 16 Labour provided by economic migrants that is generally unskilled and is used, for example, to harvest crops. The migrants generally move their residence throughout the year, following the seasonal demands for agricultural labour as different crops become ready for harvest. They may be either legally or illegally present in the host country.
forestryLogging | 20 The production of roundwood for the forest-based manufacturing industries as well as the extraction and gathering of wild growing non-wood forest products. Besides the production of timber, forestry activities result in products that undergo little processing, such as firewood, charcoal, wood chips and roundwood used in an unprocessed form (for example: as mine pit-props or for pulpwood). These activities can be carried out in natural or planted forests.
miningQuarrying | 40 The extraction of minerals occurring naturally as solids (coal and ores), liquids (petroleum) or gases (natural gas). Extraction can be achieved by different methods (for example: underground or surface mining, well operation, or seabed mining). Includes supplementary activities aimed at preparing the crude materials for marketing (for example: crushing, grinding, cleaning, drying, sorting, concentrating ores, liquefaction of natural gas and agglomeration of solid fuels. These operations are often accomplished at or near the location where the resource is extracted.
education | 850 Education at any level or for any profession, oral or written as well as by radio and television or other means of communication. It includes education by the different institutions in the regular school system at its different levels as well as adult education and literacy programmes.Also included are military schools and academies, as well as prison schools, at their respective levels.
petroleumGasExtract | 60 The production of crude petroleum, the mining and extraction of oil from oil shale and oil sands and the production of natural gas and recovery of hydrocarbon liquids. Includes the activities of operating and/or developing oil and gas field properties, for example: drilling, completing and equipping wells; operating separators, emulsion breakers, desilting equipment and field gathering lines for crude petroleum$$$$$ and all other activities in the preparation of oil and gas up to the point of shipment from the producing property. Also includes the production of oil, the mining and extraction of oil from oil shale and oil sands and the production of gas and hydrocarbon liquids, through gasification, liquefaction and pyrolysis of coal at the mine site.
recreation | 921 The provision of recreational (for example: boating, camping, fishing, or dancing), amusement (for example: amusement or theme parks) and sports activities (for example: individual or team sports). Dramatic arts, music and other arts and entertainment (for example: theatrical presentations, concerts and opera or dance productions and other stage productions) are excluded.
refugeeShelter | 883 A temporary shelter for people to live whose claim for protection has been recognised as satisfying the criteria laid down in the 1951 United Nations Convention on Refugees. Often established by governments or non-governmental organizations (such as the International Committee of the Red Cross) as temporary camps, and thus often termed a 'refugee camp'. Refugee camps are generally set up in an impromptu fashion (for example: using tents), and only designed to meet basic human needs for a short time; when civil war or other problems prevent the return of refugees, or children essentially grow up in the camps, a humanitarian crisis can result.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | featureFunction_2
Title: | FFN_2
Definition: | The purpose(s) of, or intended role(s) served by, the feature.
Multiplicity: | 0..1
Value type: | Camp_featureFunction (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
migrantLabour | 16 Labour provided by economic migrants that is generally unskilled and is used, for example, to harvest crops. The migrants generally move their residence throughout the year, following the seasonal demands for agricultural labour as different crops become ready for harvest. They may be either legally or illegally present in the host country.
forestryLogging | 20 The production of roundwood for the forest-based manufacturing industries as well as the extraction and gathering of wild growing non-wood forest products. Besides the production of timber, forestry activities result in products that undergo little processing, such as firewood, charcoal, wood chips and roundwood used in an unprocessed form (for example: as mine pit-props or for pulpwood). These activities can be carried out in natural or planted forests.
miningQuarrying | 40 The extraction of minerals occurring naturally as solids (coal and ores), liquids (petroleum) or gases (natural gas). Extraction can be achieved by different methods (for example: underground or surface mining, well operation, or seabed mining). Includes supplementary activities aimed at preparing the crude materials for marketing (for example: crushing, grinding, cleaning, drying, sorting, concentrating ores, liquefaction of natural gas and agglomeration of solid fuels. These operations are often accomplished at or near the location where the resource is extracted.
education | 850 Education at any level or for any profession, oral or written as well as by radio and television or other means of communication. It includes education by the different institutions in the regular school system at its different levels as well as adult education and literacy programmes.Also included are military schools and academies, as well as prison schools, at their respective levels.
petroleumGasExtract | 60 The production of crude petroleum, the mining and extraction of oil from oil shale and oil sands and the production of natural gas and recovery of hydrocarbon liquids. Includes the activities of operating and/or developing oil and gas field properties, for example: drilling, completing and equipping wells; operating separators, emulsion breakers, desilting equipment and field gathering lines for crude petroleum$$$$$ and all other activities in the preparation of oil and gas up to the point of shipment from the producing property. Also includes the production of oil, the mining and extraction of oil from oil shale and oil sands and the production of gas and hydrocarbon liquids, through gasification, liquefaction and pyrolysis of coal at the mine site.
recreation | 921 The provision of recreational (for example: boating, camping, fishing, or dancing), amusement (for example: amusement or theme parks) and sports activities (for example: individual or team sports). Dramatic arts, music and other arts and entertainment (for example: theatrical presentations, concerts and opera or dance productions and other stage productions) are excluded.
refugeeShelter | 883 A temporary shelter for people to live whose claim for protection has been recognised as satisfying the criteria laid down in the 1951 United Nations Convention on Refugees. Often established by governments or non-governmental organizations (such as the International Committee of the Red Cross) as temporary camps, and thus often termed a 'refugee camp'. Refugee camps are generally set up in an impromptu fashion (for example: using tents), and only designed to meet basic human needs for a short time; when civil war or other problems prevent the return of refugees, or children essentially grow up in the camps, a humanitarian crisis can result.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | featureFunction_3
Title: | FFN_3
Definition: | The purpose(s) of, or intended role(s) served by, the feature.
Multiplicity: | 0..1
Value type: | Camp_featureFunction (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
migrantLabour | 16 Labour provided by economic migrants that is generally unskilled and is used, for example, to harvest crops. The migrants generally move their residence throughout the year, following the seasonal demands for agricultural labour as different crops become ready for harvest. They may be either legally or illegally present in the host country.
forestryLogging | 20 The production of roundwood for the forest-based manufacturing industries as well as the extraction and gathering of wild growing non-wood forest products. Besides the production of timber, forestry activities result in products that undergo little processing, such as firewood, charcoal, wood chips and roundwood used in an unprocessed form (for example: as mine pit-props or for pulpwood). These activities can be carried out in natural or planted forests.
miningQuarrying | 40 The extraction of minerals occurring naturally as solids (coal and ores), liquids (petroleum) or gases (natural gas). Extraction can be achieved by different methods (for example: underground or surface mining, well operation, or seabed mining). Includes supplementary activities aimed at preparing the crude materials for marketing (for example: crushing, grinding, cleaning, drying, sorting, concentrating ores, liquefaction of natural gas and agglomeration of solid fuels. These operations are often accomplished at or near the location where the resource is extracted.
education | 850 Education at any level or for any profession, oral or written as well as by radio and television or other means of communication. It includes education by the different institutions in the regular school system at its different levels as well as adult education and literacy programmes.Also included are military schools and academies, as well as prison schools, at their respective levels.
petroleumGasExtract | 60 The production of crude petroleum, the mining and extraction of oil from oil shale and oil sands and the production of natural gas and recovery of hydrocarbon liquids. Includes the activities of operating and/or developing oil and gas field properties, for example: drilling, completing and equipping wells; operating separators, emulsion breakers, desilting equipment and field gathering lines for crude petroleum$$$$$ and all other activities in the preparation of oil and gas up to the point of shipment from the producing property. Also includes the production of oil, the mining and extraction of oil from oil shale and oil sands and the production of gas and hydrocarbon liquids, through gasification, liquefaction and pyrolysis of coal at the mine site.
recreation | 921 The provision of recreational (for example: boating, camping, fishing, or dancing), amusement (for example: amusement or theme parks) and sports activities (for example: individual or team sports). Dramatic arts, music and other arts and entertainment (for example: theatrical presentations, concerts and opera or dance productions and other stage productions) are excluded.
refugeeShelter | 883 A temporary shelter for people to live whose claim for protection has been recognised as satisfying the criteria laid down in the 1951 United Nations Convention on Refugees. Often established by governments or non-governmental organizations (such as the International Committee of the Red Cross) as temporary camps, and thus often termed a 'refugee camp'. Refugee camps are generally set up in an impromptu fashion (for example: using tents), and only designed to meet basic human needs for a short time; when civil war or other problems prevent the return of refugees, or children essentially grow up in the camps, a humanitarian crisis can result.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.baseElevation.accuracy
Title: | GEM-zI009.BEL.accuracy
Definition: | The vertical distance from a specified vertical datum to the terrain surface of or at the base of the feature.
Description: | If the feature is not supported above the surface by another feature then the base of the feature is usually located at ground or water level on the downhill/downstream side. For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). In the case of a survey marker (monument) this is usually the elevation assigned to the marker (monument).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.baseElevation.value-singleValue
Title: | GEM-zI009.BEL.value-singleValue
Definition: | The vertical distance from a specified vertical datum to the terrain surface of or at the base of the feature.
Description: | If the feature is not supported above the surface by another feature then the base of the feature is usually located at ground or water level on the downhill/downstream side. For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). In the case of a survey marker (monument) this is usually the elevation assigned to the marker (monument).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.absoluteHorizAccEvalMeth
Title: | GEM-zI009.horizCoordMetadata.AHA.absoluteHorizAccEvalMeth
Definition: | The method by which the absolute horizontal accuracy was derived.
Multiplicity: | 0..1
Value type: | HorizPosAccuracy_absoluteHorizAccEvalMeth (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
evaluationDeferred | 21 Evaluation deferred (no measurement).
geodeticSurveyAdequate | 1 Geodetic survey control - adequate sample.
geodeticSurveySmall | 2 Geodetic survey control - small sample.
photogrammAdequate | 22 Photogrammetric control - adequate sample.
photogrammSmall | 23 Photogrammetric control - small sample.
productSpecification | 15 Product specification accuracy value - assumed adequate sample.
sourceAccuracy | 13 Accuracy evaluation printed on the map sheet or the evaluation was derived from source accuracy.
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.value
Title: | GEM-zI009.horizCoordMetadata.AHA.value
Definition: | The difference between the recorded horizontal coordinates of a feature and its true position referenced to the same geodetic datum expressed as a circular error at 90 percent probability.
Description: | It may also be applied to a data set. If the data contains multiple accuracies, usually the worst accuracy which applies to 10% or more of the data is recorded.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.horizCoordMetadata.horizAccuracyCategory
Title: | GEM-zI009.horizCoordMetadata.ACC
Definition: | A general evaluation of the horizontal accuracy of the geographic position of a feature, as a category.
Multiplicity: | 0..1
Value type: | HorizCoordMetadata_horizAccuracyCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
accurate | 1 Meets specified accuracy requirements.
approximate | 2 Fails to meet specified accuracy requirements but is deemed sufficiently accurate for some uses.
doubtful | 3 Fails to meet specified accuracy requirements and is probably not sufficiently accurate for most uses.
precise | 7 Exceeds specified accuracy requirements.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.surfaceGeometry
Title: | GEM-zI009.G03
Definition: | A 2-dimensional geometric primitive, locally representing a continuous image of a region of a plane.
Description: | Its subtypes include (but are not limited to): GM_PolyhedralSurface (which aggregates GM_Polygon).
Multiplicity: | 0..1
Value type: | GM_Surface
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.absoluteVertAccEvalMeth
Title: | GEM-zI009.vertCoordMetadata.AVA.absoluteVertAccEvalMeth
Definition: | The method by which the absolute vertical accuracy was derived.
Multiplicity: | 0..1
Value type: | VertPosAccuracy_absoluteVertAccEvalMeth (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
evaluationDeferred | 21 Evaluation deferred (no measurement).
geodeticSurveyAdequate | 1 Geodetic survey control - adequate sample.
geodeticSurveySmall | 2 Geodetic survey control - small sample.
photogrammAdequate | 22 Photogrammetric control - adequate sample.
photogrammSmall | 23 Photogrammetric control - small sample.
productSpecification | 15 Product specification accuracy value - assumed adequate sample.
sourceAccuracy | 13 Accuracy evaluation printed on the map sheet or the evaluation was derived from source accuracy.
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.value
Title: | GEM-zI009.vertCoordMetadata.AVA.value
Definition: | The difference between the recorded elevation of a feature and its true elevation referenced to the same vertical datum expressed as a linear error at 90 percent probability.
Description: | It may also be applied to a data set. If the data contains multiple accuracies, usually the worst accuracy which applies to 10% or more of the data is recorded.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.vertCoordMetadata.elevationAccuracyCategory
Title: | GEM-zI009.vertCoordMetadata.ELA
Definition: | A general evaluation of the accuracy of the vertical position of a feature, as a category.
Multiplicity: | 0..1
Value type: | VertCoordMetadata_elevationAccuracyCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
accurate | 1 Meets specified accuracy requirements.
approximate | 2 Fails to meet specified accuracy requirements but is deemed sufficiently accurate for some uses.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | heightAboveSurfaceLevel.accuracy
Title: | HGT.accuracy
Definition: | The vertical distance measured from the lowest point of the base of the feature at ground or water level (downhill/downstream side) to the tallest point of the feature.
Description: | For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). Note that the feature may be supported above the surface by another feature (for example: a tower supported by a building) and as a consequence the value of the Height Above Surface Level is different (larger) than the base-to-top height of the feature (for example: supported tower) itself.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | heightAboveSurfaceLevel.value-singleValue
Title: | HGT.value-singleValue
Definition: | The vertical distance measured from the lowest point of the base of the feature at ground or water level (downhill/downstream side) to the tallest point of the feature.
Description: | For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). Note that the feature may be supported above the surface by another feature (for example: a tower supported by a building) and as a consequence the value of the Height Above Surface Level is different (larger) than the base-to-top height of the feature (for example: supported tower) itself.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | highestElevation.accuracy
Title: | ZVH.accuracy
Definition: | The elevation from a specified vertical datum to the highest point on a feature.
Description: | In the case of multiple features that may be stacked on each other (for example: a railway on a bridge, a superstructure on a building, or an aerial on a tower) the highest elevation is that of the entire feature stack. For example, the highest elevation of a church is that of its steeple and not that of the roof of the church itself. The church itself may have a height above surface level that excludes the additional height of the steeple superstructure located on the church roof.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | highestElevation.value-singleValue
Title: | ZVH.value-singleValue
Definition: | The elevation from a specified vertical datum to the highest point on a feature.
Description: | In the case of multiple features that may be stacked on each other (for example: a railway on a bridge, a superstructure on a building, or an aerial on a tower) the highest elevation is that of the entire feature stack. For example, the highest elevation of a church is that of its steeple and not that of the roof of the church itself. The church itself may have a height above surface level that excludes the additional height of the steeple superstructure located on the church roof.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | isDesignatedBy.fullName
Title: | ISDES.FNA
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.fullNameNoDiacritics
Title: | ISDES.FN1
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart except that any diacritics and special characters have been replaced with their corresponding Roman characters.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.fullNameOrdered
Title: | ISDES.FN2
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart, except that its components have been arranged into an order that facilitates alphabetic ordering and search.
Description: | The component order is such that the specific part of the name appears first, followed by an optional comma, the generic part of the name, and then finally any articles or prepositions (for example: 'Everest, Mount' or 'Mexico, Gulf of'). For some geographic names no reordering of the full name is required (for example: 'Tigrus River'). Geographic names that are believed to no longer exist are enclosed in double parenthesis, as: '(( Name ))'.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.geoNameCharacterSet
Title: | ISDES.GCS
Definition: | The character set used for the display of characters with diacritics and special characters in a geographic name.
Description: | Individual character sets include diacritics and special characters from multiple languages in the same geographic region.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geoNameCharacterSet (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
region1 | 1 Includes language-specific characters used in the Americas and Western Europe.
region2 | 2 Includes language-specific characters used in Eastern Europe.
region3 | 3 Includes language-specific characters used in Africa and the Middle East.
region4 | 4 Includes language-specific characters used in Russia and Central Asia.
region5 | 5 Includes language-specific characters used in the Asia Pacific region.
region6 | 6 Includes language-specific characters used in Vietnam.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy.geoNameDesignation
Title: | ISDES.GND
Definition: | The designation of the type of a feature with which a geographic name is associated, as used in the NGA Geographic Names Data Base (GNDB).
Description: | A designated feature type also has a (unique, single) geographic name classification.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.geographicNameType
Title: | ISDES.GNT
Definition: | The type of a geographic name based on its scope of use, quality of source and/or its transliteration status.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geographicNameType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
conventional | 1 An English name that is in widespread usage for a feature that is located in a region where English is not the official language.
historicalOriginal | 9 A historical name for a feature that remains in the original (non-Latin/Roman) script.
historicalTransliterated | 8 A historical name for a feature that has been transliterated to the Latin/Roman script as necessary.
nativeOriginal | 5 The official local name for a feature that remains in the original (non-Latin/Roman) script and is approved by the U.S. Board on Geographic Names (BGN).
nativeTransliterated | 2 The official local name for a feature that has been transliterated to the Latin/Roman script as necessary and is approved by the U.S. Board on Geographic Names (BGN).
provisional | 10 A provisional name for a feature that has been transliterated to the Latin/Roman script as necessary.
unverifiedOriginal | 7 A local name for a feature that remains in the original (non-Latin/Roman) script, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
unverifiedTransliterated | 4 A local name for a feature that has been transliterated to the Latin/Roman script as necessary, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
variantOriginal | 6 A variant or alternate name for a feature that remains in the original (non-Latin/Roman) script. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
variantTransliterated | 3 A variant or alternate name for a feature that has been transliterated to the Latin/Roman script as necessary. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy.iso15924ScriptCode
Title: | ISDES.IS1
Definition: | The International Organization for Standardization (ISO 15924) four character code that designates a script.
Description: | A script is a set of graphic characters used for the written form of one or more languages.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.languageCode
Title: | ISDES.LAN
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language or macrolanguage of the source of a geographic name.
Description: | A macrolanguage is a set of closely related language varieties (dialects) that generally have a common linguistic identity and a common written form; this may occur when there is a transitional socio-linguistic situation in which sub-communities of a single language community are diverging. The language of the geographic name source should be distinguished from the language of origin or etymology of a geographic name; for example, considering the place name 'San Jose, California' the language of the source of this geographic name may be English if it is determined from a United States map, regardless of the fact that this geographic name means 'St. Joseph, California' in Spanish.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.languageDialectCode
Title: | ISDES.LAD
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language dialect, if applicable, of the source of a geographic name.
Description: | Some languages have no (child) dialects. Each language dialect is unique to only one parent language.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.multipleOfficialNames
Title: | ISDES.MON
Definition: | An indication that a feature has more than one official, native script, geographic name.
Description: | Multiple official names may exist when a feature passes through more than one country and those multiple countries have different official names for that feature. Some countries have more than one official language and therefore may have an official name for a feature in each official language.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | isDesignatedBy.nameIdentifier
Title: | ISDES.NFN
Definition: | The unique name identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Named Feature Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.namedFeatureIdentifier
Title: | ISDES.NFI
Definition: | The unique named feature identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Name Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullName
Title: | ISDES_2.FNA
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullNameNoDiacritics
Title: | ISDES_2.FN1
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart except that any diacritics and special characters have been replaced with their corresponding Roman characters.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullNameOrdered
Title: | ISDES_2.FN2
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart, except that its components have been arranged into an order that facilitates alphabetic ordering and search.
Description: | The component order is such that the specific part of the name appears first, followed by an optional comma, the generic part of the name, and then finally any articles or prepositions (for example: 'Everest, Mount' or 'Mexico, Gulf of'). For some geographic names no reordering of the full name is required (for example: 'Tigrus River'). Geographic names that are believed to no longer exist are enclosed in double parenthesis, as: '(( Name ))'.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.geoNameCharacterSet
Title: | ISDES_2.GCS
Definition: | The character set used for the display of characters with diacritics and special characters in a geographic name.
Description: | Individual character sets include diacritics and special characters from multiple languages in the same geographic region.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geoNameCharacterSet (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
region1 | 1 Includes language-specific characters used in the Americas and Western Europe.
region2 | 2 Includes language-specific characters used in Eastern Europe.
region3 | 3 Includes language-specific characters used in Africa and the Middle East.
region4 | 4 Includes language-specific characters used in Russia and Central Asia.
region5 | 5 Includes language-specific characters used in the Asia Pacific region.
region6 | 6 Includes language-specific characters used in Vietnam.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy_2.geoNameDesignation
Title: | ISDES_2.GND
Definition: | The designation of the type of a feature with which a geographic name is associated, as used in the NGA Geographic Names Data Base (GNDB).
Description: | A designated feature type also has a (unique, single) geographic name classification.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.geographicNameType
Title: | ISDES_2.GNT
Definition: | The type of a geographic name based on its scope of use, quality of source and/or its transliteration status.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geographicNameType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
conventional | 1 An English name that is in widespread usage for a feature that is located in a region where English is not the official language.
historicalOriginal | 9 A historical name for a feature that remains in the original (non-Latin/Roman) script.
historicalTransliterated | 8 A historical name for a feature that has been transliterated to the Latin/Roman script as necessary.
nativeOriginal | 5 The official local name for a feature that remains in the original (non-Latin/Roman) script and is approved by the U.S. Board on Geographic Names (BGN).
nativeTransliterated | 2 The official local name for a feature that has been transliterated to the Latin/Roman script as necessary and is approved by the U.S. Board on Geographic Names (BGN).
provisional | 10 A provisional name for a feature that has been transliterated to the Latin/Roman script as necessary.
unverifiedOriginal | 7 A local name for a feature that remains in the original (non-Latin/Roman) script, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
unverifiedTransliterated | 4 A local name for a feature that has been transliterated to the Latin/Roman script as necessary, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
variantOriginal | 6 A variant or alternate name for a feature that remains in the original (non-Latin/Roman) script. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
variantTransliterated | 3 A variant or alternate name for a feature that has been transliterated to the Latin/Roman script as necessary. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy_2.iso15924ScriptCode
Title: | ISDES_2.IS1
Definition: | The International Organization for Standardization (ISO 15924) four character code that designates a script.
Description: | A script is a set of graphic characters used for the written form of one or more languages.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.languageCode
Title: | ISDES_2.LAN
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language or macrolanguage of the source of a geographic name.
Description: | A macrolanguage is a set of closely related language varieties (dialects) that generally have a common linguistic identity and a common written form; this may occur when there is a transitional socio-linguistic situation in which sub-communities of a single language community are diverging. The language of the geographic name source should be distinguished from the language of origin or etymology of a geographic name; for example, considering the place name 'San Jose, California' the language of the source of this geographic name may be English if it is determined from a United States map, regardless of the fact that this geographic name means 'St. Joseph, California' in Spanish.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.languageDialectCode
Title: | ISDES_2.LAD
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language dialect, if applicable, of the source of a geographic name.
Description: | Some languages have no (child) dialects. Each language dialect is unique to only one parent language.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.multipleOfficialNames
Title: | ISDES_2.MON
Definition: | An indication that a feature has more than one official, native script, geographic name.
Description: | Multiple official names may exist when a feature passes through more than one country and those multiple countries have different official names for that feature. Some countries have more than one official language and therefore may have an official name for a feature in each official language.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | isDesignatedBy_2.nameIdentifier
Title: | ISDES_2.NFN
Definition: | The unique name identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Named Feature Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.namedFeatureIdentifier
Title: | ISDES_2.NFI
Definition: | The unique named feature identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Name Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | metadata.dataQualityStatement
Title: | MD0.DQS
Definition: | A narrative or other textual description that records a general assessment of the quality of a resource (for example: a data instance, a data set or a data processing activity).
Description: | The quality of a data resource is dependent on the data providers knowledge regarding the lineage of the data and the processes that have been used to transform that data. No restriction is placed on the length of the statement.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | metadata.delineationKnown
Title: | MD0.COD
Definition: | An indication that the delineation (for example: limits and information) of a feature is known.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | metadata.existenceCertaintyCat
Title: | MD0.COE
Definition: | A general evaluation of the quality of a feature assessment, as a category.
Multiplicity: | 0..1
Value type: | FeatureMetadata_existenceCertaintyCat (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
definite | 1 A feature whose existence has been confirmed by a trusted source.
doubtful | 2 A feature whose existence has been reported and was not able to be confirmed, but which is assumed to be present for reasons of safety.
reported | 3 A feature whose existence has been reported but not confirmed.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | metadata.surveyCoverageCategory
Title: | MD0.SUR
Definition: | A general evaluation of the coverage quality of a survey, as a category.
Description: | See possibly accompanying Attribute: 'Position Quality Category' for additional survey-related information.
Multiplicity: | 0..1
Value type: | FeatureMetadata_surveyCoverageCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
inadequatelySurveyed | 2 Surveyed, but not with complete coverage and/or not to established standards.
surveyed | 1 Surveyed with complete coverage and to established standards. Survey implies a regular, controlled survey of any date.
unsurveyed | 3 Survey data either does not exist or is very poor in coverage and/or quality.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | nomadicSeasonalLocation
Title: | STL
Definition: | The season(s) in which a nomadic people are camped at a given location.
Multiplicity: | 0..1
Value type: | Camp_nomadicSeasonalLocation (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
winter | 1 The fourth and coldest season of the year, coming between autumn and spring; reckoned astronomically from the winter solstice to the vernal equinox. For example, in the northern hemisphere, nominally from December 21 to March 21.
summer | 2 The second and warmest season of the year, coming between spring and autumn; reckoned astronomically from the summer solstice to the autumnal equinox. For example, in the northern hemisphere, nominally from June 21 to September 21.
spring | 3 The first season of the year, coming between winter and summer, reckoned astronomically from the vernal equinox to the summer solstice. For example, in the northern hemisphere, nominally from March 21 to June 21.
autumn | 4 The third season of the year, coming between summer and winter, reckoned astronomically from the autumnal equinox to the winter solstice. For example, in the northern hemisphere, nominally from September 21 to December 21.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | nomadicSeasonalLocation_2
Title: | STL_2
Definition: | The season(s) in which a nomadic people are camped at a given location.
Multiplicity: | 0..1
Value type: | Camp_nomadicSeasonalLocation (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
winter | 1 The fourth and coldest season of the year, coming between autumn and spring; reckoned astronomically from the winter solstice to the vernal equinox. For example, in the northern hemisphere, nominally from December 21 to March 21.
summer | 2 The second and warmest season of the year, coming between spring and autumn; reckoned astronomically from the summer solstice to the autumnal equinox. For example, in the northern hemisphere, nominally from June 21 to September 21.
spring | 3 The first season of the year, coming between winter and summer, reckoned astronomically from the vernal equinox to the summer solstice. For example, in the northern hemisphere, nominally from March 21 to June 21.
autumn | 4 The third season of the year, coming between summer and winter, reckoned astronomically from the autumnal equinox to the winter solstice. For example, in the northern hemisphere, nominally from September 21 to December 21.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | nomadicSeasonalLocation_3
Title: | STL_3
Definition: | The season(s) in which a nomadic people are camped at a given location.
Multiplicity: | 0..1
Value type: | Camp_nomadicSeasonalLocation (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
winter | 1 The fourth and coldest season of the year, coming between autumn and spring; reckoned astronomically from the winter solstice to the vernal equinox. For example, in the northern hemisphere, nominally from December 21 to March 21.
summer | 2 The second and warmest season of the year, coming between spring and autumn; reckoned astronomically from the summer solstice to the autumnal equinox. For example, in the northern hemisphere, nominally from June 21 to September 21.
spring | 3 The first season of the year, coming between winter and summer, reckoned astronomically from the vernal equinox to the summer solstice. For example, in the northern hemisphere, nominally from March 21 to June 21.
autumn | 4 The third season of the year, coming between summer and winter, reckoned astronomically from the autumnal equinox to the winter solstice. For example, in the northern hemisphere, nominally from September 21 to December 21.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | physicalCondition
Title: | PCF
Definition: | The physical condition of a man-made structure, as a whole, including the inside and/or outside of the structure and any contained and/or associated equipment.
Description: | The physical condition applies to any phase of the life cycle of a man-made structure from construction to destruction. Examples of man-made structures include roads, canals, buildings, towers, aerodromes and facilities.
Multiplicity: | 0..1
Value type: | Camp_physicalCondition (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
construction | 1 The man-made structure is being built or undergoing renovation or repair. Incorporates site preparations, building of new construction and the renovation or repair of existing structures.
intact | 2 The man-made structure is complete and intact. The man-made structure may or may not be in operation or use.
unmaintained | 3 The man-made structure is left in place to deteriorate. The man-made structure has been abandoned and no maintenance or repairs are being carried out. While the structure is physically intact, no signs of operation are visible.
damaged | 4 The man-made structure is damaged. Damage may be a consequence of accident, military action, or natural disaster. The damaged man-made structure can be repaired.
dismantled | 5 The man-made structure has undergone a systematic selective removal of components. Low value components and/or equipment may remain. The man-made structure cannot be repaired without a great deal of time and effort.
destroyed | 6 The man-made structure has undergone complete destruction and is in a state of total disrepair. Destruction may be a consequence of military action, natural disaster, planned demolition or a long period of no maintenance. A destroyed man-made structure can only be restored by complete reconstruction.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | predominantFeatureHeight-singleValue
Title: | PFH-singleValue
Definition: | The predominant height (the height of at least 50 percent) of the feature measured from the lowest point of the base at ground or water level (downhill side/downstream side).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | settlementPattern
Title: | USP
Definition: | The pattern of settlement of an urban area based on the most frequently occurring geometric configuration (pattern) of streets and/or canals.
Multiplicity: | 0..1
Value type: | Camp_settlementPattern (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
rectangularRegular | 2 The streets form an intersecting grid pattern of approximately regularly spaced lines at right angles to each other.
rectangularButIrregular | 3 The streets form a discontinuous intersecting grid pattern of approximately regularly spaced lines at right angles to each other. Street discontinuities are often created to form small urban parks, or to discourage through-traffic in a residential neighborhood; the consequence is blocky irregularities in the overall pattern.
curvilinear | 4 The streets follow a planned pattern of curves and irregularities designed to discourage through traffic and ensure increased privacy. Usually only found in residential neighborhoods.
radialRegular | 6 The streets tend to radiate out from a central point in a somewhat evenly spaced pattern in all directions similar to the spokes of a wheel; side streets connecting to the radials tend to be unevenly spaced and to connect only a few of the radials instead of going completely around.
radialButIrregular | 7 The streets tend to radiate out from a central point in an unevenly spaced pattern in all directions similar to the spokes of a wheel; side streets connecting to the radials tend to be unevenly spaced and to connect only a few of the radials instead of going completely around.
mixedRectCurvilinear | 9 The streets follow a mix of rectangular and curvilinear patterns.
mixedRectangularRadial | 10 The streets follow a mix of rectangular and radial patterns.
mixedRadialCurvilinear | 11 The streets follow a mix of radial and curvilinear patterns.
linear | 13 There is a single main street perhaps with a short paralleling side street, or it stretches out in both directions along two main intersecting roads (in outline configured as a cross). Sometimes referred to a strip development and common on the edge of expanding urban areas or in rural areas where the main thoroughfare or intersecting roads are the only ones paved or otherwise improved.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | specifiedDomainValues
Title: | OTH
Definition: | One or more intended attribute domain values for one or more enumeration or codelist attributes that are not currently valid members of their respective attribute ranges.
Description: | The actual attribute domain values may have been previously, or may become in the future, valid members of the attribute domain range.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | structMatType
Title: | MCC
Definition: | The primary type(s) of material composing a feature, exclusive of the surface.
Description: | The basis for 'primary' may be, for example, compositional dominance or structural organization.
Multiplicity: | 0..1
Value type: | Camp_structMatType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
metal | 64 Any of the class of substances that are characteristically lustrous, ductile, fusible, malleable solids and are good conductors of heat and electricity. For example, gold, silver, copper, iron, lead, tin, and certain alloys (as brass and bronze).
plastic | 74 Any of a large class of substances which are polymers based on synthetic resins or modified natural polymers. May be moulded, extruded, or cast while soft or liquid, and then set into a rigid or slightly elastic form, usually by heating or cooling.
vegetation | 113 Plants collectively, especially those dominating a particular area or habitat.
wood | 117 The hard, compact, fibrous substance of which the roots, trunks, and branches of trees and shrubs consist. Consists largely of secondary xylem, which forms the strengthening and water-transporting tissue of the plant.
hideTextile | 153 Any thin, flexible sheet material consisting of cured animal hides and/or textiles. The textile may be based on a mixture of natural (for example: cotton) and/or man-made (for example: nylon) fibres.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | structMatType_2
Title: | MCC_2
Definition: | The primary type(s) of material composing a feature, exclusive of the surface.
Description: | The basis for 'primary' may be, for example, compositional dominance or structural organization.
Multiplicity: | 0..1
Value type: | Camp_structMatType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
metal | 64 Any of the class of substances that are characteristically lustrous, ductile, fusible, malleable solids and are good conductors of heat and electricity. For example, gold, silver, copper, iron, lead, tin, and certain alloys (as brass and bronze).
plastic | 74 Any of a large class of substances which are polymers based on synthetic resins or modified natural polymers. May be moulded, extruded, or cast while soft or liquid, and then set into a rigid or slightly elastic form, usually by heating or cooling.
vegetation | 113 Plants collectively, especially those dominating a particular area or habitat.
wood | 117 The hard, compact, fibrous substance of which the roots, trunks, and branches of trees and shrubs consist. Consists largely of secondary xylem, which forms the strengthening and water-transporting tissue of the plant.
hideTextile | 153 Any thin, flexible sheet material consisting of cured animal hides and/or textiles. The textile may be based on a mixture of natural (for example: cotton) and/or man-made (for example: nylon) fibres.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | structMatType_3
Title: | MCC_3
Definition: | The primary type(s) of material composing a feature, exclusive of the surface.
Description: | The basis for 'primary' may be, for example, compositional dominance or structural organization.
Multiplicity: | 0..1
Value type: | Camp_structMatType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
metal | 64 Any of the class of substances that are characteristically lustrous, ductile, fusible, malleable solids and are good conductors of heat and electricity. For example, gold, silver, copper, iron, lead, tin, and certain alloys (as brass and bronze).
plastic | 74 Any of a large class of substances which are polymers based on synthetic resins or modified natural polymers. May be moulded, extruded, or cast while soft or liquid, and then set into a rigid or slightly elastic form, usually by heating or cooling.
vegetation | 113 Plants collectively, especially those dominating a particular area or habitat.
wood | 117 The hard, compact, fibrous substance of which the roots, trunks, and branches of trees and shrubs consist. Consists largely of secondary xylem, which forms the strengthening and water-transporting tissue of the plant.
hideTextile | 153 Any thin, flexible sheet material consisting of cured animal hides and/or textiles. The textile may be based on a mixture of natural (for example: cotton) and/or man-made (for example: nylon) fibres.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | structureDensity-singleValue
Title: | DMS-singleValue
Definition: | The density of structures in an area.
Description: | The number of structures in the area are counted and divided by the total area. Major wings may be counted as separate buildings provided there are significant changes in roof directions from the main building.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | uniqueEntityIdentifier
Title: | UFI
Definition: | The globally unique and persistent identifier of an entity (for example: feature or event) instance as specified by a Uniform Resource Name (URN) in accordance with the Internet Engineering Task Force (IETF) RFC2396 and RFC2141.
Description: | It is based on the Uniform Resource Identifier (URI), a compact string of characters for identifying an abstract or physical resource. The term 'Uniform Resource Name' (URN) refers to the subset of URI that are required to remain globally unique and persistent even when the resource ceases to exist or becomes unavailable. The URN is drawn from one of a set of defined namespaces, each of which has its own set name structure and assignment procedures.
Multiplicity: | 1
Value type: | CharacterString
## Attribute: back to top
Name: | universalUniqueIdentifier
Title: | UUI
Definition: | The Universal Unique Identifier (UUID) that is assigned to a feature in order to uniquely identify it for the purpose of maintaining relationships between features (relational database) and version control.
Description: | UUIDs are defined in ITU-T Rec. X.667 |||||||||||||||||||||||||||||||| ISO/IEC 9834-8.
Multiplicity: | 1
Value type: | CharacterString