# Feature type: FiringRange_S

## Package: MiscellaneousCulturalFeatures
## Title: FA015_S
## Definition: A site designated for the purpose of discharging firearms or detonating munitions.
## Type: Feature type
## Overview of characteristics:
Attributes and association roles
Name | Type | Multiplicity
--- | --- | ---
angleOfOrientation | Real | 0..1
containedInStructure | BooleanWithONINA | 0..1
controllingAuthority | FiringRange_controllingAuthority | 0..1
facilityOperationalStatus | FiringRange_facilityOperationalStatus | 0..1
featureFunction | FiringRange_featureFunction | 0..1
featureFunction_2 | FiringRange_featureFunction | 0..1
featureFunction_3 | FiringRange_featureFunction | 0..1
geometry-surfaceGeometryInfo.baseElevation.accuracy | Real | 0..1
geometry-surfaceGeometryInfo.baseElevation.value-singleValue | Real | 0..1
geometry-surfaceGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.absoluteHorizAccEvalMeth | HorizPosAccuracy_absoluteHorizAccEvalMeth | 0..1
geometry-surfaceGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.value | Real | 0..1
geometry-surfaceGeometryInfo.horizCoordMetadata.horizAccuracyCategory | HorizCoordMetadata_horizAccuracyCategory | 0..1
geometry-surfaceGeometryInfo.surfaceGeometry | GM_Surface | 0..1
geometry-surfaceGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.absoluteVertAccEvalMeth | VertPosAccuracy_absoluteVertAccEvalMeth | 0..1
geometry-surfaceGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.value | Real | 0..1
geometry-surfaceGeometryInfo.vertCoordMetadata.elevationAccuracyCategory | VertCoordMetadata_elevationAccuracyCategory | 0..1
heightAboveSurfaceLevel.accuracy | Real | 0..1
heightAboveSurfaceLevel.value-singleValue | Real | 0..1
highestElevation.accuracy | Real | 0..1
highestElevation.value-singleValue | Real | 0..1
hydrographicBaseHeight.value-singleValue | Real | 0..1
isDesignatedBy.fullName | CharacterString | 0..1
isDesignatedBy.fullNameNoDiacritics | CharacterString | 0..1
isDesignatedBy.fullNameOrdered | CharacterString | 0..1
isDesignatedBy.geoNameCharacterSet | GeoNameInfo_geoNameCharacterSet | 0..1
isDesignatedBy.geoNameDesignation | CharacterString | 0..1
isDesignatedBy.geographicNameType | GeoNameInfo_geographicNameType | 0..1
isDesignatedBy.iso15924ScriptCode | CharacterString | 0..1
isDesignatedBy.languageCode | CharacterString | 0..1
isDesignatedBy.languageDialectCode | CharacterString | 0..1
isDesignatedBy.multipleOfficialNames | BooleanWithONINA | 0..1
isDesignatedBy.nameIdentifier | CharacterString | 0..1
isDesignatedBy.namedFeatureIdentifier | CharacterString | 0..1
isDesignatedBy_2.fullName | CharacterString | 0..1
isDesignatedBy_2.fullNameNoDiacritics | CharacterString | 0..1
isDesignatedBy_2.fullNameOrdered | CharacterString | 0..1
isDesignatedBy_2.geoNameCharacterSet | GeoNameInfo_geoNameCharacterSet | 0..1
isDesignatedBy_2.geoNameDesignation | CharacterString | 0..1
isDesignatedBy_2.geographicNameType | GeoNameInfo_geographicNameType | 0..1
isDesignatedBy_2.iso15924ScriptCode | CharacterString | 0..1
isDesignatedBy_2.languageCode | CharacterString | 0..1
isDesignatedBy_2.languageDialectCode | CharacterString | 0..1
isDesignatedBy_2.multipleOfficialNames | BooleanWithONINA | 0..1
isDesignatedBy_2.nameIdentifier | CharacterString | 0..1
isDesignatedBy_2.namedFeatureIdentifier | CharacterString | 0..1
locationRefToShoreline | FiringRange_locationRefToShoreline | 0..1
metadata.dataQualityStatement | CharacterString | 0..1
metadata.delineationKnown | BooleanWithONINA | 0..1
metadata.existenceCertaintyCat | FeatureMetadata_existenceCertaintyCat | 0..1
metadata.surveyCoverageCategory | FeatureMetadata_surveyCoverageCategory | 0..1
militaryServiceBranch | FiringRange_militaryServiceBranch | 0..1
monitored | BooleanWithONINA | 0..1
permanent | BooleanWithONINA | 0..1
physicalCondition | FiringRange_physicalCondition | 0..1
relativeLevel | FiringRange_relativeLevel | 0..1
specifiedDomainValues | CharacterString | 0..1
structMatType | FiringRange_structMatType | 0..1
structMatType_2 | FiringRange_structMatType | 0..1
structMatType_3 | FiringRange_structMatType | 0..1
uniqueEntityIdentifier | CharacterString | 1
universalUniqueIdentifier | CharacterString | 1
weaponsRangeType | FiringRange_weaponsRangeType | 0..1
weaponsRangeType_2 | FiringRange_weaponsRangeType | 0..1
weaponsRangeType_3 | FiringRange_weaponsRangeType | 0..1
## Attribute: back to top
Name: | angleOfOrientation
Title: | AOO
Definition: | The angular distance in the horizontal plane measured from true north (0 degrees) clockwise to the major axis of the feature.
Description: | If the feature is square, the axis 0 up to 90 degrees is recorded. If the feature is circular, 360 degrees is recorded.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | containedInStructure
Title: | CWS
Definition: | The object is located within a structure (for example: a building).
Description: | For example, a slipway inside of a boat house.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | controllingAuthority
Title: | CAA
Definition: | The controlling authority responsible for a facility or site.
Description: | Controlling authorities may be distinguished by organizational level (for example: national, sub-national, or military district) and/or type (for example: private or public).
Multiplicity: | 0..1
Value type: | FiringRange_controllingAuthority (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
private | 3 Administered by an individual or corporation, rather than a State or a public body.
military | 5 An armed force constituted under the laws of a State.
civilian | 16 An administrative unit not associated with an armed force.
jointMilitaryCivilian | 7 An administrative body composed of both military and civil authorities. Often created during times of civil unrest or war and intended to be of a temporary nature.
public | 17 Administered on behalf all members of a community, rather than restricted to an individual or corporation.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | facilityOperationalStatus
Title: | COS
Definition: | The status of operation of a man-made structure, as a whole.
Description: | Includes actual operations, operational capability, and planned or proposed man-made structures.
Multiplicity: | 0..1
Value type: | FiringRange_facilityOperationalStatus (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
intermittent | 2 Operations are intended to be continuous but may be interrupted on a scheduled basis.
nonOperational | 4 Not in operation due to it being non-functional and operation is not scheduled to be restored.
operational | 13 Fully capable of operation. The schedule of operations may be indeterminate or unknown.
notInOperation | 8 Fully functional and ready for operation however has not been certified or commissioned for such use. The operational capacity may not be authorized for various reasons, such as newly installed and not yet commissioned or certified, or operational but has been taken out of service for non-technical reasons, awaiting certification or commissioning status.
partiallyOperational | 14 Functional, but operating with only partial capability for some reason. Parts of the man-made structure are not in operation; or, the operation is running below capacity.
planned | 6 Future operations are scheduled.
temporarilyNonOperational | 9 Temporarily not in operation due to it being non-functional and operation is scheduled to be restored. Usually an unscheduled loss of operation.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | featureFunction
Title: | FFN
Definition: | The purpose(s) of, or intended role(s) served by, the feature.
Multiplicity: | 0..1
Value type: | FiringRange_featureFunction (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
defenceActivities | 835 The administration, supervision and/or operation of military defence affairs and land, sea, air and space defence forces.
lawEnforcement | 841 The administration and operation of regular and auxiliary police forces involved in the prevention, investigation, apprehension, or detention of individuals suspected or convicted of offenses against the criminal laws. May include auxiliary duties (for example: traffic regulation, alien registration, or maintenance of arrest records).
recreation | 921 The provision of recreational (for example: boating, camping, fishing, or dancing), amusement (for example: amusement or theme parks) and sports activities (for example: individual or team sports). Dramatic arts, music and other arts and entertainment (for example: theatrical presentations, concerts and opera or dance productions and other stage productions) are excluded.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | featureFunction_2
Title: | FFN_2
Definition: | The purpose(s) of, or intended role(s) served by, the feature.
Multiplicity: | 0..1
Value type: | FiringRange_featureFunction (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
defenceActivities | 835 The administration, supervision and/or operation of military defence affairs and land, sea, air and space defence forces.
lawEnforcement | 841 The administration and operation of regular and auxiliary police forces involved in the prevention, investigation, apprehension, or detention of individuals suspected or convicted of offenses against the criminal laws. May include auxiliary duties (for example: traffic regulation, alien registration, or maintenance of arrest records).
recreation | 921 The provision of recreational (for example: boating, camping, fishing, or dancing), amusement (for example: amusement or theme parks) and sports activities (for example: individual or team sports). Dramatic arts, music and other arts and entertainment (for example: theatrical presentations, concerts and opera or dance productions and other stage productions) are excluded.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | featureFunction_3
Title: | FFN_3
Definition: | The purpose(s) of, or intended role(s) served by, the feature.
Multiplicity: | 0..1
Value type: | FiringRange_featureFunction (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
defenceActivities | 835 The administration, supervision and/or operation of military defence affairs and land, sea, air and space defence forces.
lawEnforcement | 841 The administration and operation of regular and auxiliary police forces involved in the prevention, investigation, apprehension, or detention of individuals suspected or convicted of offenses against the criminal laws. May include auxiliary duties (for example: traffic regulation, alien registration, or maintenance of arrest records).
recreation | 921 The provision of recreational (for example: boating, camping, fishing, or dancing), amusement (for example: amusement or theme parks) and sports activities (for example: individual or team sports). Dramatic arts, music and other arts and entertainment (for example: theatrical presentations, concerts and opera or dance productions and other stage productions) are excluded.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.baseElevation.accuracy
Title: | GEM-zI009.BEL.accuracy
Definition: | The vertical distance from a specified vertical datum to the terrain surface of or at the base of the feature.
Description: | If the feature is not supported above the surface by another feature then the base of the feature is usually located at ground or water level on the downhill/downstream side. For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). In the case of a survey marker (monument) this is usually the elevation assigned to the marker (monument).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.baseElevation.value-singleValue
Title: | GEM-zI009.BEL.value-singleValue
Definition: | The vertical distance from a specified vertical datum to the terrain surface of or at the base of the feature.
Description: | If the feature is not supported above the surface by another feature then the base of the feature is usually located at ground or water level on the downhill/downstream side. For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). In the case of a survey marker (monument) this is usually the elevation assigned to the marker (monument).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.absoluteHorizAccEvalMeth
Title: | GEM-zI009.horizCoordMetadata.AHA.absoluteHorizAccEvalMeth
Definition: | The method by which the absolute horizontal accuracy was derived.
Multiplicity: | 0..1
Value type: | HorizPosAccuracy_absoluteHorizAccEvalMeth (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
evaluationDeferred | 21 Evaluation deferred (no measurement).
geodeticSurveyAdequate | 1 Geodetic survey control - adequate sample.
geodeticSurveySmall | 2 Geodetic survey control - small sample.
photogrammAdequate | 22 Photogrammetric control - adequate sample.
photogrammSmall | 23 Photogrammetric control - small sample.
productSpecification | 15 Product specification accuracy value - assumed adequate sample.
sourceAccuracy | 13 Accuracy evaluation printed on the map sheet or the evaluation was derived from source accuracy.
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.value
Title: | GEM-zI009.horizCoordMetadata.AHA.value
Definition: | The difference between the recorded horizontal coordinates of a feature and its true position referenced to the same geodetic datum expressed as a circular error at 90 percent probability.
Description: | It may also be applied to a data set. If the data contains multiple accuracies, usually the worst accuracy which applies to 10% or more of the data is recorded.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.horizCoordMetadata.horizAccuracyCategory
Title: | GEM-zI009.horizCoordMetadata.ACC
Definition: | A general evaluation of the horizontal accuracy of the geographic position of a feature, as a category.
Multiplicity: | 0..1
Value type: | HorizCoordMetadata_horizAccuracyCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
accurate | 1 Meets specified accuracy requirements.
approximate | 2 Fails to meet specified accuracy requirements but is deemed sufficiently accurate for some uses.
doubtful | 3 Fails to meet specified accuracy requirements and is probably not sufficiently accurate for most uses.
precise | 7 Exceeds specified accuracy requirements.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.surfaceGeometry
Title: | GEM-zI009.G03
Definition: | A 2-dimensional geometric primitive, locally representing a continuous image of a region of a plane.
Description: | Its subtypes include (but are not limited to): GM_PolyhedralSurface (which aggregates GM_Polygon).
Multiplicity: | 0..1
Value type: | GM_Surface
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.absoluteVertAccEvalMeth
Title: | GEM-zI009.vertCoordMetadata.AVA.absoluteVertAccEvalMeth
Definition: | The method by which the absolute vertical accuracy was derived.
Multiplicity: | 0..1
Value type: | VertPosAccuracy_absoluteVertAccEvalMeth (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
evaluationDeferred | 21 Evaluation deferred (no measurement).
geodeticSurveyAdequate | 1 Geodetic survey control - adequate sample.
geodeticSurveySmall | 2 Geodetic survey control - small sample.
photogrammAdequate | 22 Photogrammetric control - adequate sample.
photogrammSmall | 23 Photogrammetric control - small sample.
productSpecification | 15 Product specification accuracy value - assumed adequate sample.
sourceAccuracy | 13 Accuracy evaluation printed on the map sheet or the evaluation was derived from source accuracy.
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.value
Title: | GEM-zI009.vertCoordMetadata.AVA.value
Definition: | The difference between the recorded elevation of a feature and its true elevation referenced to the same vertical datum expressed as a linear error at 90 percent probability.
Description: | It may also be applied to a data set. If the data contains multiple accuracies, usually the worst accuracy which applies to 10% or more of the data is recorded.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-surfaceGeometryInfo.vertCoordMetadata.elevationAccuracyCategory
Title: | GEM-zI009.vertCoordMetadata.ELA
Definition: | A general evaluation of the accuracy of the vertical position of a feature, as a category.
Multiplicity: | 0..1
Value type: | VertCoordMetadata_elevationAccuracyCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
accurate | 1 Meets specified accuracy requirements.
approximate | 2 Fails to meet specified accuracy requirements but is deemed sufficiently accurate for some uses.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | heightAboveSurfaceLevel.accuracy
Title: | HGT.accuracy
Definition: | The vertical distance measured from the lowest point of the base of the feature at ground or water level (downhill/downstream side) to the tallest point of the feature.
Description: | For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). Note that the feature may be supported above the surface by another feature (for example: a tower supported by a building) and as a consequence the value of the Height Above Surface Level is different (larger) than the base-to-top height of the feature (for example: supported tower) itself.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | heightAboveSurfaceLevel.value-singleValue
Title: | HGT.value-singleValue
Definition: | The vertical distance measured from the lowest point of the base of the feature at ground or water level (downhill/downstream side) to the tallest point of the feature.
Description: | For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). Note that the feature may be supported above the surface by another feature (for example: a tower supported by a building) and as a consequence the value of the Height Above Surface Level is different (larger) than the base-to-top height of the feature (for example: supported tower) itself.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | highestElevation.accuracy
Title: | ZVH.accuracy
Definition: | The elevation from a specified vertical datum to the highest point on a feature.
Description: | In the case of multiple features that may be stacked on each other (for example: a railway on a bridge, a superstructure on a building, or an aerial on a tower) the highest elevation is that of the entire feature stack. For example, the highest elevation of a church is that of its steeple and not that of the roof of the church itself. The church itself may have a height above surface level that excludes the additional height of the steeple superstructure located on the church roof.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | highestElevation.value-singleValue
Title: | ZVH.value-singleValue
Definition: | The elevation from a specified vertical datum to the highest point on a feature.
Description: | In the case of multiple features that may be stacked on each other (for example: a railway on a bridge, a superstructure on a building, or an aerial on a tower) the highest elevation is that of the entire feature stack. For example, the highest elevation of a church is that of its steeple and not that of the roof of the church itself. The church itself may have a height above surface level that excludes the additional height of the steeple superstructure located on the church roof.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | hydrographicBaseHeight.value-singleValue
Title: | HBH.value-singleValue
Definition: | The height from a specified sounding datum to the bottom or base of a feature (for example: the base of a lighthouse).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | isDesignatedBy.fullName
Title: | ISDES.FNA
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.fullNameNoDiacritics
Title: | ISDES.FN1
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart except that any diacritics and special characters have been replaced with their corresponding Roman characters.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.fullNameOrdered
Title: | ISDES.FN2
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart, except that its components have been arranged into an order that facilitates alphabetic ordering and search.
Description: | The component order is such that the specific part of the name appears first, followed by an optional comma, the generic part of the name, and then finally any articles or prepositions (for example: 'Everest, Mount' or 'Mexico, Gulf of'). For some geographic names no reordering of the full name is required (for example: 'Tigrus River'). Geographic names that are believed to no longer exist are enclosed in double parenthesis, as: '(( Name ))'.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.geoNameCharacterSet
Title: | ISDES.GCS
Definition: | The character set used for the display of characters with diacritics and special characters in a geographic name.
Description: | Individual character sets include diacritics and special characters from multiple languages in the same geographic region.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geoNameCharacterSet (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
region1 | 1 Includes language-specific characters used in the Americas and Western Europe.
region2 | 2 Includes language-specific characters used in Eastern Europe.
region3 | 3 Includes language-specific characters used in Africa and the Middle East.
region4 | 4 Includes language-specific characters used in Russia and Central Asia.
region5 | 5 Includes language-specific characters used in the Asia Pacific region.
region6 | 6 Includes language-specific characters used in Vietnam.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy.geoNameDesignation
Title: | ISDES.GND
Definition: | The designation of the type of a feature with which a geographic name is associated, as used in the NGA Geographic Names Data Base (GNDB).
Description: | A designated feature type also has a (unique, single) geographic name classification.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.geographicNameType
Title: | ISDES.GNT
Definition: | The type of a geographic name based on its scope of use, quality of source and/or its transliteration status.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geographicNameType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
conventional | 1 An English name that is in widespread usage for a feature that is located in a region where English is not the official language.
historicalOriginal | 9 A historical name for a feature that remains in the original (non-Latin/Roman) script.
historicalTransliterated | 8 A historical name for a feature that has been transliterated to the Latin/Roman script as necessary.
nativeOriginal | 5 The official local name for a feature that remains in the original (non-Latin/Roman) script and is approved by the U.S. Board on Geographic Names (BGN).
nativeTransliterated | 2 The official local name for a feature that has been transliterated to the Latin/Roman script as necessary and is approved by the U.S. Board on Geographic Names (BGN).
provisional | 10 A provisional name for a feature that has been transliterated to the Latin/Roman script as necessary.
unverifiedOriginal | 7 A local name for a feature that remains in the original (non-Latin/Roman) script, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
unverifiedTransliterated | 4 A local name for a feature that has been transliterated to the Latin/Roman script as necessary, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
variantOriginal | 6 A variant or alternate name for a feature that remains in the original (non-Latin/Roman) script. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
variantTransliterated | 3 A variant or alternate name for a feature that has been transliterated to the Latin/Roman script as necessary. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy.iso15924ScriptCode
Title: | ISDES.IS1
Definition: | The International Organization for Standardization (ISO 15924) four character code that designates a script.
Description: | A script is a set of graphic characters used for the written form of one or more languages.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.languageCode
Title: | ISDES.LAN
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language or macrolanguage of the source of a geographic name.
Description: | A macrolanguage is a set of closely related language varieties (dialects) that generally have a common linguistic identity and a common written form; this may occur when there is a transitional socio-linguistic situation in which sub-communities of a single language community are diverging. The language of the geographic name source should be distinguished from the language of origin or etymology of a geographic name; for example, considering the place name 'San Jose, California' the language of the source of this geographic name may be English if it is determined from a United States map, regardless of the fact that this geographic name means 'St. Joseph, California' in Spanish.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.languageDialectCode
Title: | ISDES.LAD
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language dialect, if applicable, of the source of a geographic name.
Description: | Some languages have no (child) dialects. Each language dialect is unique to only one parent language.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.multipleOfficialNames
Title: | ISDES.MON
Definition: | An indication that a feature has more than one official, native script, geographic name.
Description: | Multiple official names may exist when a feature passes through more than one country and those multiple countries have different official names for that feature. Some countries have more than one official language and therefore may have an official name for a feature in each official language.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | isDesignatedBy.nameIdentifier
Title: | ISDES.NFN
Definition: | The unique name identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Named Feature Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.namedFeatureIdentifier
Title: | ISDES.NFI
Definition: | The unique named feature identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Name Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullName
Title: | ISDES_2.FNA
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullNameNoDiacritics
Title: | ISDES_2.FN1
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart except that any diacritics and special characters have been replaced with their corresponding Roman characters.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullNameOrdered
Title: | ISDES_2.FN2
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart, except that its components have been arranged into an order that facilitates alphabetic ordering and search.
Description: | The component order is such that the specific part of the name appears first, followed by an optional comma, the generic part of the name, and then finally any articles or prepositions (for example: 'Everest, Mount' or 'Mexico, Gulf of'). For some geographic names no reordering of the full name is required (for example: 'Tigrus River'). Geographic names that are believed to no longer exist are enclosed in double parenthesis, as: '(( Name ))'.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.geoNameCharacterSet
Title: | ISDES_2.GCS
Definition: | The character set used for the display of characters with diacritics and special characters in a geographic name.
Description: | Individual character sets include diacritics and special characters from multiple languages in the same geographic region.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geoNameCharacterSet (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
region1 | 1 Includes language-specific characters used in the Americas and Western Europe.
region2 | 2 Includes language-specific characters used in Eastern Europe.
region3 | 3 Includes language-specific characters used in Africa and the Middle East.
region4 | 4 Includes language-specific characters used in Russia and Central Asia.
region5 | 5 Includes language-specific characters used in the Asia Pacific region.
region6 | 6 Includes language-specific characters used in Vietnam.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy_2.geoNameDesignation
Title: | ISDES_2.GND
Definition: | The designation of the type of a feature with which a geographic name is associated, as used in the NGA Geographic Names Data Base (GNDB).
Description: | A designated feature type also has a (unique, single) geographic name classification.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.geographicNameType
Title: | ISDES_2.GNT
Definition: | The type of a geographic name based on its scope of use, quality of source and/or its transliteration status.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geographicNameType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
conventional | 1 An English name that is in widespread usage for a feature that is located in a region where English is not the official language.
historicalOriginal | 9 A historical name for a feature that remains in the original (non-Latin/Roman) script.
historicalTransliterated | 8 A historical name for a feature that has been transliterated to the Latin/Roman script as necessary.
nativeOriginal | 5 The official local name for a feature that remains in the original (non-Latin/Roman) script and is approved by the U.S. Board on Geographic Names (BGN).
nativeTransliterated | 2 The official local name for a feature that has been transliterated to the Latin/Roman script as necessary and is approved by the U.S. Board on Geographic Names (BGN).
provisional | 10 A provisional name for a feature that has been transliterated to the Latin/Roman script as necessary.
unverifiedOriginal | 7 A local name for a feature that remains in the original (non-Latin/Roman) script, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
unverifiedTransliterated | 4 A local name for a feature that has been transliterated to the Latin/Roman script as necessary, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
variantOriginal | 6 A variant or alternate name for a feature that remains in the original (non-Latin/Roman) script. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
variantTransliterated | 3 A variant or alternate name for a feature that has been transliterated to the Latin/Roman script as necessary. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy_2.iso15924ScriptCode
Title: | ISDES_2.IS1
Definition: | The International Organization for Standardization (ISO 15924) four character code that designates a script.
Description: | A script is a set of graphic characters used for the written form of one or more languages.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.languageCode
Title: | ISDES_2.LAN
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language or macrolanguage of the source of a geographic name.
Description: | A macrolanguage is a set of closely related language varieties (dialects) that generally have a common linguistic identity and a common written form; this may occur when there is a transitional socio-linguistic situation in which sub-communities of a single language community are diverging. The language of the geographic name source should be distinguished from the language of origin or etymology of a geographic name; for example, considering the place name 'San Jose, California' the language of the source of this geographic name may be English if it is determined from a United States map, regardless of the fact that this geographic name means 'St. Joseph, California' in Spanish.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.languageDialectCode
Title: | ISDES_2.LAD
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language dialect, if applicable, of the source of a geographic name.
Description: | Some languages have no (child) dialects. Each language dialect is unique to only one parent language.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.multipleOfficialNames
Title: | ISDES_2.MON
Definition: | An indication that a feature has more than one official, native script, geographic name.
Description: | Multiple official names may exist when a feature passes through more than one country and those multiple countries have different official names for that feature. Some countries have more than one official language and therefore may have an official name for a feature in each official language.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | isDesignatedBy_2.nameIdentifier
Title: | ISDES_2.NFN
Definition: | The unique name identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Named Feature Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.namedFeatureIdentifier
Title: | ISDES_2.NFI
Definition: | The unique named feature identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Name Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | locationRefToShoreline
Title: | SRL
Definition: | The location of an object in relation to a land water boundary.
Multiplicity: | 0..1
Value type: | FiringRange_locationRefToShoreline (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
offshore | 1 Located offshore. The object is always wet.
inland | 2 Located inland of the land water boundary. The object is always dry.
atShoreline | 3 Straddles the land water boundary. The object may be wet or dry at various times.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | metadata.dataQualityStatement
Title: | MD0.DQS
Definition: | A narrative or other textual description that records a general assessment of the quality of a resource (for example: a data instance, a data set or a data processing activity).
Description: | The quality of a data resource is dependent on the data providers knowledge regarding the lineage of the data and the processes that have been used to transform that data. No restriction is placed on the length of the statement.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | metadata.delineationKnown
Title: | MD0.COD
Definition: | An indication that the delineation (for example: limits and information) of a feature is known.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | metadata.existenceCertaintyCat
Title: | MD0.COE
Definition: | A general evaluation of the quality of a feature assessment, as a category.
Multiplicity: | 0..1
Value type: | FeatureMetadata_existenceCertaintyCat (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
definite | 1 A feature whose existence has been confirmed by a trusted source.
doubtful | 2 A feature whose existence has been reported and was not able to be confirmed, but which is assumed to be present for reasons of safety.
reported | 3 A feature whose existence has been reported but not confirmed.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | metadata.surveyCoverageCategory
Title: | MD0.SUR
Definition: | A general evaluation of the coverage quality of a survey, as a category.
Description: | See possibly accompanying Attribute: 'Position Quality Category' for additional survey-related information.
Multiplicity: | 0..1
Value type: | FeatureMetadata_surveyCoverageCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
inadequatelySurveyed | 2 Surveyed, but not with complete coverage and/or not to established standards.
surveyed | 1 Surveyed with complete coverage and to established standards. Survey implies a regular, controlled survey of any date.
unsurveyed | 3 Survey data either does not exist or is very poor in coverage and/or quality.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | militaryServiceBranch
Title: | YSU
Definition: | The branch of the armed forces of a nation.
Description: | May also be applied to similar organizations following military discipline (for example: a coastguard).
Multiplicity: | 0..1
Value type: | FiringRange_militaryServiceBranch (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
airForce | 1 The branch of a country's armed forces which conducts operations primarily by means of aircraft.
army | 2 The branch of a country's armed forces which conducts operations on land.
coastguard | 3 A naval force employed to guard the coast, and often responsible for the safety, order, and operation of marine traffic in neighbouring waters.
marines | 4 A body of soldiers trained to serve at sea, or on shore under specified circumstances.
navy | 5 The branch of a country's armed forces which conducts operations at sea and/or using sea-based capabilities, including both ships and ship-based aircraft. Navy operations are supported by land-based capabilities including ports and maintenance systems typically also belonging to the Navy.
joint | 7 An organization in which elements of two or more military departments (for example: a navy and an air force) participate.
airNationalGuard | 8 A military reserve force which conducts operations primarily by means of aircraft. A military reserve force is a military organization composed of residents of a country who combine a military role or career with a civilian career. They are not normally kept under arms and their main role is to be available to fight when a nation mobilizes for total war or to defend against invasion. Military reserve forces may be employed in non-military settings (for example: disaster relief).
armyNationalGuard | 9 A military reserve force equipped to fight on land. A military reserve force is a military organization composed of residents of a country who combine a military role or career with a civilian career. They are not normally kept under arms and their main role is be available to fight when a nation mobilizes for total war or to defend against invasion. Military reserve forces may be employed in non-military settings (for example: disaster relief).
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | monitored
Title: | MOS
Definition: | An indication that a feature is actively monitored.
Description: | For example, attended or watched over by personnel.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | permanent
Title: | PRM
Definition: | An indication that a feature is permanent.
Description: | Temporary features last, or are meant to last, for a limited time only.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | physicalCondition
Title: | PCF
Definition: | The physical condition of a man-made structure, as a whole, including the inside and/or outside of the structure and any contained and/or associated equipment.
Description: | The physical condition applies to any phase of the life cycle of a man-made structure from construction to destruction. Examples of man-made structures include roads, canals, buildings, towers, aerodromes and facilities.
Multiplicity: | 0..1
Value type: | FiringRange_physicalCondition (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
construction | 1 The man-made structure is being built or undergoing renovation or repair. Incorporates site preparations, building of new construction and the renovation or repair of existing structures.
damaged | 4 The man-made structure is damaged. Damage may be a consequence of accident, military action, or natural disaster. The damaged man-made structure can be repaired.
destroyed | 6 The man-made structure has undergone complete destruction and is in a state of total disrepair. Destruction may be a consequence of military action, natural disaster, planned demolition or a long period of no maintenance. A destroyed man-made structure can only be restored by complete reconstruction.
dismantled | 5 The man-made structure has undergone a systematic selective removal of components. Low value components and/or equipment may remain. The man-made structure cannot be repaired without a great deal of time and effort.
intact | 2 The man-made structure is complete and intact. The man-made structure may or may not be in operation or use.
unmaintained | 3 The man-made structure is left in place to deteriorate. The man-made structure has been abandoned and no maintenance or repairs are being carried out. While the structure is physically intact, no signs of operation are visible.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | relativeLevel
Title: | RLE
Definition: | The relationship of the elevation of the terrain surface of or at the base of the feature and that of the surrounding terrain.
Description: | The terrain may be either dry or submerged (for example: a waterbody bottom).
Multiplicity: | 0..1
Value type: | FiringRange_relativeLevel (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
raised | 1 A localized area of significantly higher elevation than that of the surrounding terrain. For example, an embankment, a berm, a ridge, a terrain mound, and a fill.
level | 2 An area of similar or identical elevation to that of the surrounding terrain.
depressed | 3 A localized area of significantly lower elevation than that of the surrounding terrain. For example, a terrain depression, a gully, a moat and a terrain cut for a road, railway and/or canal.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | specifiedDomainValues
Title: | OTH
Definition: | One or more intended attribute domain values for one or more enumeration or codelist attributes that are not currently valid members of their respective attribute ranges.
Description: | The actual attribute domain values may have been previously, or may become in the future, valid members of the attribute domain range.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | structMatType
Title: | MCC
Definition: | The primary type(s) of material composing a feature, exclusive of the surface.
Description: | The basis for 'primary' may be, for example, compositional dominance or structural organization.
Multiplicity: | 0..1
Value type: | FiringRange_structMatType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
boulders | 8 Large water- or weather-worn stones.
brick | 9 Clay kneaded, moulded, and baked or sun-dried, used as a building material.
concrete | 21 A heavy-duty building material made from a mixture of broken stone or gravel, sand, cement, and water, that forms a stonelike mass on hardening.
masonry | 62 Building materials (for example: stone, brick, concrete, hollow-tile, concrete block, gypsum block, or other similar building units or materials and/or a combination of the same) bonded together with mortar to form a structure (for example: a wall, a pier, or a buttress).
prestressedConcrete | 77 Reinforced concrete in which internal stresses have been introduced to reduce potential tensile stress in the concrete resulting from loads.
reinforcedConcrete | 83 Poured concrete containing steel bars or metal netting to increase its tensile strength.
rock | 84 Stones of any size.
soil | 104 The material comprising the thin top layer of much of the Earth's land surface, composed of fragmented rock particles with humus, water, and air.
wood | 117 The hard, compact, fibrous substance of which the roots, trunks, and branches of trees and shrubs consist. Consists largely of secondary xylem, which forms the strengthening and water-transporting tissue of the plant.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | structMatType_2
Title: | MCC_2
Definition: | The primary type(s) of material composing a feature, exclusive of the surface.
Description: | The basis for 'primary' may be, for example, compositional dominance or structural organization.
Multiplicity: | 0..1
Value type: | FiringRange_structMatType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
boulders | 8 Large water- or weather-worn stones.
brick | 9 Clay kneaded, moulded, and baked or sun-dried, used as a building material.
concrete | 21 A heavy-duty building material made from a mixture of broken stone or gravel, sand, cement, and water, that forms a stonelike mass on hardening.
masonry | 62 Building materials (for example: stone, brick, concrete, hollow-tile, concrete block, gypsum block, or other similar building units or materials and/or a combination of the same) bonded together with mortar to form a structure (for example: a wall, a pier, or a buttress).
prestressedConcrete | 77 Reinforced concrete in which internal stresses have been introduced to reduce potential tensile stress in the concrete resulting from loads.
reinforcedConcrete | 83 Poured concrete containing steel bars or metal netting to increase its tensile strength.
rock | 84 Stones of any size.
soil | 104 The material comprising the thin top layer of much of the Earth's land surface, composed of fragmented rock particles with humus, water, and air.
wood | 117 The hard, compact, fibrous substance of which the roots, trunks, and branches of trees and shrubs consist. Consists largely of secondary xylem, which forms the strengthening and water-transporting tissue of the plant.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | structMatType_3
Title: | MCC_3
Definition: | The primary type(s) of material composing a feature, exclusive of the surface.
Description: | The basis for 'primary' may be, for example, compositional dominance or structural organization.
Multiplicity: | 0..1
Value type: | FiringRange_structMatType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
boulders | 8 Large water- or weather-worn stones.
brick | 9 Clay kneaded, moulded, and baked or sun-dried, used as a building material.
concrete | 21 A heavy-duty building material made from a mixture of broken stone or gravel, sand, cement, and water, that forms a stonelike mass on hardening.
masonry | 62 Building materials (for example: stone, brick, concrete, hollow-tile, concrete block, gypsum block, or other similar building units or materials and/or a combination of the same) bonded together with mortar to form a structure (for example: a wall, a pier, or a buttress).
prestressedConcrete | 77 Reinforced concrete in which internal stresses have been introduced to reduce potential tensile stress in the concrete resulting from loads.
reinforcedConcrete | 83 Poured concrete containing steel bars or metal netting to increase its tensile strength.
rock | 84 Stones of any size.
soil | 104 The material comprising the thin top layer of much of the Earth's land surface, composed of fragmented rock particles with humus, water, and air.
wood | 117 The hard, compact, fibrous substance of which the roots, trunks, and branches of trees and shrubs consist. Consists largely of secondary xylem, which forms the strengthening and water-transporting tissue of the plant.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | uniqueEntityIdentifier
Title: | UFI
Definition: | The globally unique and persistent identifier of an entity (for example: feature or event) instance as specified by a Uniform Resource Name (URN) in accordance with the Internet Engineering Task Force (IETF) RFC2396 and RFC2141.
Description: | It is based on the Uniform Resource Identifier (URI), a compact string of characters for identifying an abstract or physical resource. The term 'Uniform Resource Name' (URN) refers to the subset of URI that are required to remain globally unique and persistent even when the resource ceases to exist or becomes unavailable. The URN is drawn from one of a set of defined namespaces, each of which has its own set name structure and assignment procedures.
Multiplicity: | 1
Value type: | CharacterString
## Attribute: back to top
Name: | universalUniqueIdentifier
Title: | UUI
Definition: | The Universal Unique Identifier (UUID) that is assigned to a feature in order to uniquely identify it for the purpose of maintaining relationships between features (relational database) and version control.
Description: | UUIDs are defined in ITU-T Rec. X.667 |||||||||||||||||||||||||||||||| ISO/IEC 9834-8.
Multiplicity: | 1
Value type: | CharacterString
## Attribute: back to top
Name: | weaponsRangeType
Title: | FRT
Definition: | The type of a weapons range based on its intended use(s).
Multiplicity: | 0..1
Value type: | FiringRange_weaponsRangeType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
smallArms | 1 Suitable for training with and testing pistols, rifles, machine guns, and other small calibre weapons.
tank | 2 Suitable for training with and testing the large-caliber high-velocity main gun of a battle tank, as well as other weapons found on armoured vehicles. The main gun is usually capable of firing kinetic energy penetrators, high explosive anti-tank rounds, and in some cases guided missiles. Such practice may include maneuver as well as discharge of weapons.
fieldArtillery | 3 Suitable for training with and testing large-calibre field artillery weapons (for example: a howitzer or a cannon).
grenade | 4 Suitable for training with and testing grenades. A grenade is a small explosive or chemical bomb detonated by a fuse and which may be thrown by hand or launched from a special device attached to a rifle or carbine.
demolitionArea | 5 An area allocated for breaking up of structures and/or equipment (for example: destruction of arms by international agreement) by explosive blasting.
impactArea | 6 An area allocated for bombardment during the live firing of weapons.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | weaponsRangeType_2
Title: | FRT_2
Definition: | The type of a weapons range based on its intended use(s).
Multiplicity: | 0..1
Value type: | FiringRange_weaponsRangeType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
smallArms | 1 Suitable for training with and testing pistols, rifles, machine guns, and other small calibre weapons.
tank | 2 Suitable for training with and testing the large-caliber high-velocity main gun of a battle tank, as well as other weapons found on armoured vehicles. The main gun is usually capable of firing kinetic energy penetrators, high explosive anti-tank rounds, and in some cases guided missiles. Such practice may include maneuver as well as discharge of weapons.
fieldArtillery | 3 Suitable for training with and testing large-calibre field artillery weapons (for example: a howitzer or a cannon).
grenade | 4 Suitable for training with and testing grenades. A grenade is a small explosive or chemical bomb detonated by a fuse and which may be thrown by hand or launched from a special device attached to a rifle or carbine.
demolitionArea | 5 An area allocated for breaking up of structures and/or equipment (for example: destruction of arms by international agreement) by explosive blasting.
impactArea | 6 An area allocated for bombardment during the live firing of weapons.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | weaponsRangeType_3
Title: | FRT_3
Definition: | The type of a weapons range based on its intended use(s).
Multiplicity: | 0..1
Value type: | FiringRange_weaponsRangeType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
smallArms | 1 Suitable for training with and testing pistols, rifles, machine guns, and other small calibre weapons.
tank | 2 Suitable for training with and testing the large-caliber high-velocity main gun of a battle tank, as well as other weapons found on armoured vehicles. The main gun is usually capable of firing kinetic energy penetrators, high explosive anti-tank rounds, and in some cases guided missiles. Such practice may include maneuver as well as discharge of weapons.
fieldArtillery | 3 Suitable for training with and testing large-calibre field artillery weapons (for example: a howitzer or a cannon).
grenade | 4 Suitable for training with and testing grenades. A grenade is a small explosive or chemical bomb detonated by a fuse and which may be thrown by hand or launched from a special device attached to a rifle or carbine.
demolitionArea | 5 An area allocated for breaking up of structures and/or equipment (for example: destruction of arms by international agreement) by explosive blasting.
impactArea | 6 An area allocated for bombardment during the live firing of weapons.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other