# Feature type: Runway_C

## Package: AircraftMovementSurfaces
## Title: GB055_C
## Definition: A defined rectangular area on a land aerodrome prepared for the landing and take-off of aircraft.
## Type: Feature type
## Overview of characteristics:
Attributes and association roles
Name | Type | Multiplicity
--- | --- | ---
aerodromeSurfaceStatus | AerodromeMoveArea_aerodromeSurfaceStatus | 0..1
aircraftMaxDemoLcnSpan | CharacterString | 0..1
availabilityCategory | AerodromeMoveArea_availabilityCategory | 0..1
controllingAuthority | Runway_controllingAuthority | 0..1
facilityOperationalStatus | AerodromeMoveArea_facilityOperationalStatus | 0..1
geometry-curveGeometryInfo.area | Real | 0..1
geometry-curveGeometryInfo.baseElevation.accuracy | Real | 0..1
geometry-curveGeometryInfo.baseElevation.value-singleValue | Real | 0..1
geometry-curveGeometryInfo.curveGeometry | GM_Curve | 0..1
geometry-curveGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.absoluteHorizAccEvalMeth | HorizPosAccuracy_absoluteHorizAccEvalMeth | 0..1
geometry-curveGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.value | Real | 0..1
geometry-curveGeometryInfo.horizCoordMetadata.horizAccuracyCategory | HorizCoordMetadata_horizAccuracyCategory | 0..1
geometry-curveGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.absoluteVertAccEvalMeth | VertPosAccuracy_absoluteVertAccEvalMeth | 0..1
geometry-curveGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.value | Real | 0..1
geometry-curveGeometryInfo.vertCoordMetadata.elevationAccuracyCategory | VertCoordMetadata_elevationAccuracyCategory | 0..1
geometry-curveGeometryInfo.width-singleValue | Real | 0..1
highestElevation.accuracy | Real | 0..1
highestElevation.value-singleValue | Real | 0..1
isDesignatedBy.fullName | CharacterString | 0..1
isDesignatedBy.fullNameNoDiacritics | CharacterString | 0..1
isDesignatedBy.fullNameOrdered | CharacterString | 0..1
isDesignatedBy.geoNameCharacterSet | GeoNameInfo_geoNameCharacterSet | 0..1
isDesignatedBy.geoNameDesignation | CharacterString | 0..1
isDesignatedBy.geographicNameType | GeoNameInfo_geographicNameType | 0..1
isDesignatedBy.iso15924ScriptCode | CharacterString | 0..1
isDesignatedBy.languageCode | CharacterString | 0..1
isDesignatedBy.languageDialectCode | CharacterString | 0..1
isDesignatedBy.multipleOfficialNames | BooleanWithONINA | 0..1
isDesignatedBy.nameIdentifier | CharacterString | 0..1
isDesignatedBy.namedFeatureIdentifier | CharacterString | 0..1
isDesignatedBy_2.fullName | CharacterString | 0..1
isDesignatedBy_2.fullNameNoDiacritics | CharacterString | 0..1
isDesignatedBy_2.fullNameOrdered | CharacterString | 0..1
isDesignatedBy_2.geoNameCharacterSet | GeoNameInfo_geoNameCharacterSet | 0..1
isDesignatedBy_2.geoNameDesignation | CharacterString | 0..1
isDesignatedBy_2.geographicNameType | GeoNameInfo_geographicNameType | 0..1
isDesignatedBy_2.iso15924ScriptCode | CharacterString | 0..1
isDesignatedBy_2.languageCode | CharacterString | 0..1
isDesignatedBy_2.languageDialectCode | CharacterString | 0..1
isDesignatedBy_2.multipleOfficialNames | BooleanWithONINA | 0..1
isDesignatedBy_2.nameIdentifier | CharacterString | 0..1
isDesignatedBy_2.namedFeatureIdentifier | CharacterString | 0..1
metadata.dataQualityStatement | CharacterString | 0..1
metadata.delineationKnown | BooleanWithONINA | 0..1
metadata.existenceCertaintyCat | FeatureMetadata_existenceCertaintyCat | 0..1
metadata.surveyCoverageCategory | FeatureMetadata_surveyCoverageCategory | 0..1
movementAreaEntryClearance | Real | 0..1
pavementInfo.aeroMoveAreaSurfaceCat | AerodromePavementInfo_aeroMoveAreaSurfaceCat | 0..1
pavementInfo.aeroMoveAreaSurfacePrep | AerodromePavementInfo_aeroMoveAreaSurfacePrep | 0..1
pavementInfo.aeroMoveAreaSurfacePrep_2 | AerodromePavementInfo_aeroMoveAreaSurfacePrep | 0..1
pavementInfo.aeroMoveAreaSurfacePrep_3 | AerodromePavementInfo_aeroMoveAreaSurfacePrep | 0..1
pavementInfo.aeroPavementFuncStatus | AerodromePavementInfo_aeroPavementFuncStatus | 0..1
pavementInfo.loadClassificationNumber | Integer | 0..1
pavementInfo.pavementClassNumber | Integer | 0..1
pavementInfo.pavementTypeForPcnDeterm | AerodromePavementInfo_pavementTypeForPcnDeterm | 0..1
pavementInfo.pcnEvaluationMethod | AerodromePavementInfo_pcnEvaluationMethod | 0..1
pavementInfo.pcnMaxAllowTirePressCat | AerodromePavementInfo_pcnMaxAllowTirePressCat | 0..1
pavementInfo.pcnPavementSubStrengthCat | AerodromePavementInfo_pcnPavementSubStrengthCat | 0..1
pavementInfo.runwayObservedLoading | CharacterString | 0..1
permanent | BooleanWithONINA | 0..1
physicalCondition | AerodromeMoveArea_physicalCondition | 0..1
runwayBearingStrength | Real | 0..1
runwayMidpointElevation | Real | 0..1
specifiedDomainValues | CharacterString | 0..1
supportedByBridgeSpan | BooleanWithONINA | 0..1
uniqueEntityIdentifier | CharacterString | 1
universalUniqueIdentifier | CharacterString | 1
## Attribute: back to top
Name: | aerodromeSurfaceStatus
Title: | AXS
Definition: | The operational status of an aerodrome movement area, as a category.
Description: | For example: serviceable, unserviceable, closed, or work-in-progress.
Multiplicity: | 0..1
Value type: | AerodromeMoveArea_aerodromeSurfaceStatus (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
closed | 1 Access is officially prohibited.
open | 2 Access is officially permitted.
workInProgress | 3 The surface is under construction and is therefore not capable of supporting aircraft operations.
parkedDisabledAircraft | 4 Aircraft may be parked on the movement surface limiting operations.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | aircraftMaxDemoLcnSpan
Title: | MDS
Definition: | The largest wingspan aircraft of the highest Load Classification Number (LCN) known to have used a runway in the last five years.
Description: | An aircraft with a shorter wingspan and the higher LCN will be identified in preference to an aircraft with a longer wingspan but lower LCN.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | availabilityCategory
Title: | ACG
Definition: | The reported availability of a product, service, feature, or facility, as a category.
Multiplicity: | 0..1
Value type: | AerodromeMoveArea_availabilityCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
confirmedAvailable | 2 The product, service, feature, or facility is confirmed to be available.
notAvailable | 1 The product, service, feature, or facility is confirmed to be unavailable.
unconfirmedAvailable | 3 The product, service, feature, or facility may be available, but this has not been confirmed.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | controllingAuthority
Title: | CAA
Definition: | The controlling authority responsible for a facility or site.
Description: | Controlling authorities may be distinguished by organizational level (for example: national, sub-national, or military district) and/or type (for example: private or public).
Multiplicity: | 0..1
Value type: | Runway_controllingAuthority (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
private | 3 Administered by an individual or corporation, rather than a State or a public body.
military | 5 An armed force constituted under the laws of a State.
jointMilitaryCivilian | 7 An administrative body composed of both military and civil authorities. Often created during times of civil unrest or war and intended to be of a temporary nature.
civilian | 16 An administrative unit not associated with an armed force.
public | 17 Administered on behalf all members of a community, rather than restricted to an individual or corporation.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | facilityOperationalStatus
Title: | COS
Definition: | The status of operation of a man-made structure, as a whole.
Description: | Includes actual operations, operational capability, and planned or proposed man-made structures.
Multiplicity: | 0..1
Value type: | AerodromeMoveArea_facilityOperationalStatus (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
nonOperational | 4 Not in operation due to it being non-functional and operation is not scheduled to be restored.
temporarilyNonOperational | 9 Temporarily not in operation due to it being non-functional and operation is scheduled to be restored. Usually an unscheduled loss of operation.
planned | 6 Future operations are scheduled.
notInOperation | 8 Fully functional and ready for operation however has not been certified or commissioned for such use. The operational capacity may not be authorized for various reasons, such as newly installed and not yet commissioned or certified, or operational but has been taken out of service for non-technical reasons, awaiting certification or commissioning status.
operational | 13 Fully capable of operation. The schedule of operations may be indeterminate or unknown.
partiallyOperational | 14 Functional, but operating with only partial capability for some reason. Parts of the man-made structure are not in operation; or, the operation is running below capacity.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | geometry-curveGeometryInfo.area
Title: | GEM-zI008.ARA
Definition: | The area within the delineation of the feature.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-curveGeometryInfo.baseElevation.accuracy
Title: | GEM-zI008.BEL.accuracy
Definition: | The vertical distance from a specified vertical datum to the terrain surface of or at the base of the feature.
Description: | If the feature is not supported above the surface by another feature then the base of the feature is usually located at ground or water level on the downhill/downstream side. For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). In the case of a survey marker (monument) this is usually the elevation assigned to the marker (monument).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-curveGeometryInfo.baseElevation.value-singleValue
Title: | GEM-zI008.BEL.value-singleValue
Definition: | The vertical distance from a specified vertical datum to the terrain surface of or at the base of the feature.
Description: | If the feature is not supported above the surface by another feature then the base of the feature is usually located at ground or water level on the downhill/downstream side. For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). In the case of a survey marker (monument) this is usually the elevation assigned to the marker (monument).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-curveGeometryInfo.curveGeometry
Title: | GEM-zI008.G02
Definition: | A 1-dimensional geometric primitive, representing the continuous image of a line.
Description: | Its subtypes include (but are not limited to): GM_LineString, GM_LineSegment, GM_GeodesicString, GM_Geodesic, GM_ArcString, and GM_Arc.
Multiplicity: | 0..1
Value type: | GM_Curve
## Attribute: back to top
Name: | geometry-curveGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.absoluteHorizAccEvalMeth
Title: | GEM-zI008.horizCoordMetadata.AHA.absoluteHorizAccEvalMeth
Definition: | The method by which the absolute horizontal accuracy was derived.
Multiplicity: | 0..1
Value type: | HorizPosAccuracy_absoluteHorizAccEvalMeth (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
evaluationDeferred | 21 Evaluation deferred (no measurement).
geodeticSurveyAdequate | 1 Geodetic survey control - adequate sample.
geodeticSurveySmall | 2 Geodetic survey control - small sample.
photogrammAdequate | 22 Photogrammetric control - adequate sample.
photogrammSmall | 23 Photogrammetric control - small sample.
productSpecification | 15 Product specification accuracy value - assumed adequate sample.
sourceAccuracy | 13 Accuracy evaluation printed on the map sheet or the evaluation was derived from source accuracy.
## Attribute: back to top
Name: | geometry-curveGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.value
Title: | GEM-zI008.horizCoordMetadata.AHA.value
Definition: | The difference between the recorded horizontal coordinates of a feature and its true position referenced to the same geodetic datum expressed as a circular error at 90 percent probability.
Description: | It may also be applied to a data set. If the data contains multiple accuracies, usually the worst accuracy which applies to 10% or more of the data is recorded.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-curveGeometryInfo.horizCoordMetadata.horizAccuracyCategory
Title: | GEM-zI008.horizCoordMetadata.ACC
Definition: | A general evaluation of the horizontal accuracy of the geographic position of a feature, as a category.
Multiplicity: | 0..1
Value type: | HorizCoordMetadata_horizAccuracyCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
accurate | 1 Meets specified accuracy requirements.
approximate | 2 Fails to meet specified accuracy requirements but is deemed sufficiently accurate for some uses.
doubtful | 3 Fails to meet specified accuracy requirements and is probably not sufficiently accurate for most uses.
precise | 7 Exceeds specified accuracy requirements.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | geometry-curveGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.absoluteVertAccEvalMeth
Title: | GEM-zI008.vertCoordMetadata.AVA.absoluteVertAccEvalMeth
Definition: | The method by which the absolute vertical accuracy was derived.
Multiplicity: | 0..1
Value type: | VertPosAccuracy_absoluteVertAccEvalMeth (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
evaluationDeferred | 21 Evaluation deferred (no measurement).
geodeticSurveyAdequate | 1 Geodetic survey control - adequate sample.
geodeticSurveySmall | 2 Geodetic survey control - small sample.
photogrammAdequate | 22 Photogrammetric control - adequate sample.
photogrammSmall | 23 Photogrammetric control - small sample.
productSpecification | 15 Product specification accuracy value - assumed adequate sample.
sourceAccuracy | 13 Accuracy evaluation printed on the map sheet or the evaluation was derived from source accuracy.
## Attribute: back to top
Name: | geometry-curveGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.value
Title: | GEM-zI008.vertCoordMetadata.AVA.value
Definition: | The difference between the recorded elevation of a feature and its true elevation referenced to the same vertical datum expressed as a linear error at 90 percent probability.
Description: | It may also be applied to a data set. If the data contains multiple accuracies, usually the worst accuracy which applies to 10% or more of the data is recorded.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-curveGeometryInfo.vertCoordMetadata.elevationAccuracyCategory
Title: | GEM-zI008.vertCoordMetadata.ELA
Definition: | A general evaluation of the accuracy of the vertical position of a feature, as a category.
Multiplicity: | 0..1
Value type: | VertCoordMetadata_elevationAccuracyCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
accurate | 1 Meets specified accuracy requirements.
approximate | 2 Fails to meet specified accuracy requirements but is deemed sufficiently accurate for some uses.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | geometry-curveGeometryInfo.width-singleValue
Title: | GEM-zI008.WID-singleValue
Definition: | The dimension of a feature taken perpendicular to its primary alignment of use and generally in the horizontal plane.
Description: | The primary alignment of a feature is its established direction of flow or use (for example: a road, a power line right-of-way, a river, rapid, and/or a bridge). A feature-specific rule may apply. In the case of a bridge, the width is the distance perpendicular to the bridge centre-line and generally in the horizontal plane. In the case of a dam, the width is the distance perpendicular to (across the) the dam crest. If no such direction of flow or use exists then (1) if the feature is irregular in shape its width is taken perpendicular to the direction of its greatest horizontal dimension (see Attribute: 'Greatest Horizontal Extent'), else (2) if the feature is regular in shape then a shape-specific rule may apply: for a rectangular feature, the length of the shorter axis; for a round feature, the diameter.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | highestElevation.accuracy
Title: | ZVH.accuracy
Definition: | The elevation from a specified vertical datum to the highest point on a feature.
Description: | In the case of multiple features that may be stacked on each other (for example: a railway on a bridge, a superstructure on a building, or an aerial on a tower) the highest elevation is that of the entire feature stack. For example, the highest elevation of a church is that of its steeple and not that of the roof of the church itself. The church itself may have a height above surface level that excludes the additional height of the steeple superstructure located on the church roof.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | highestElevation.value-singleValue
Title: | ZVH.value-singleValue
Definition: | The elevation from a specified vertical datum to the highest point on a feature.
Description: | In the case of multiple features that may be stacked on each other (for example: a railway on a bridge, a superstructure on a building, or an aerial on a tower) the highest elevation is that of the entire feature stack. For example, the highest elevation of a church is that of its steeple and not that of the roof of the church itself. The church itself may have a height above surface level that excludes the additional height of the steeple superstructure located on the church roof.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | isDesignatedBy.fullName
Title: | ISDES.FNA
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.fullNameNoDiacritics
Title: | ISDES.FN1
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart except that any diacritics and special characters have been replaced with their corresponding Roman characters.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.fullNameOrdered
Title: | ISDES.FN2
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart, except that its components have been arranged into an order that facilitates alphabetic ordering and search.
Description: | The component order is such that the specific part of the name appears first, followed by an optional comma, the generic part of the name, and then finally any articles or prepositions (for example: 'Everest, Mount' or 'Mexico, Gulf of'). For some geographic names no reordering of the full name is required (for example: 'Tigrus River'). Geographic names that are believed to no longer exist are enclosed in double parenthesis, as: '(( Name ))'.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.geoNameCharacterSet
Title: | ISDES.GCS
Definition: | The character set used for the display of characters with diacritics and special characters in a geographic name.
Description: | Individual character sets include diacritics and special characters from multiple languages in the same geographic region.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geoNameCharacterSet (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
region1 | 1 Includes language-specific characters used in the Americas and Western Europe.
region2 | 2 Includes language-specific characters used in Eastern Europe.
region3 | 3 Includes language-specific characters used in Africa and the Middle East.
region4 | 4 Includes language-specific characters used in Russia and Central Asia.
region5 | 5 Includes language-specific characters used in the Asia Pacific region.
region6 | 6 Includes language-specific characters used in Vietnam.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy.geoNameDesignation
Title: | ISDES.GND
Definition: | The designation of the type of a feature with which a geographic name is associated, as used in the NGA Geographic Names Data Base (GNDB).
Description: | A designated feature type also has a (unique, single) geographic name classification.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.geographicNameType
Title: | ISDES.GNT
Definition: | The type of a geographic name based on its scope of use, quality of source and/or its transliteration status.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geographicNameType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
conventional | 1 An English name that is in widespread usage for a feature that is located in a region where English is not the official language.
historicalOriginal | 9 A historical name for a feature that remains in the original (non-Latin/Roman) script.
historicalTransliterated | 8 A historical name for a feature that has been transliterated to the Latin/Roman script as necessary.
nativeOriginal | 5 The official local name for a feature that remains in the original (non-Latin/Roman) script and is approved by the U.S. Board on Geographic Names (BGN).
nativeTransliterated | 2 The official local name for a feature that has been transliterated to the Latin/Roman script as necessary and is approved by the U.S. Board on Geographic Names (BGN).
provisional | 10 A provisional name for a feature that has been transliterated to the Latin/Roman script as necessary.
unverifiedOriginal | 7 A local name for a feature that remains in the original (non-Latin/Roman) script, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
unverifiedTransliterated | 4 A local name for a feature that has been transliterated to the Latin/Roman script as necessary, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
variantOriginal | 6 A variant or alternate name for a feature that remains in the original (non-Latin/Roman) script. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
variantTransliterated | 3 A variant or alternate name for a feature that has been transliterated to the Latin/Roman script as necessary. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy.iso15924ScriptCode
Title: | ISDES.IS1
Definition: | The International Organization for Standardization (ISO 15924) four character code that designates a script.
Description: | A script is a set of graphic characters used for the written form of one or more languages.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.languageCode
Title: | ISDES.LAN
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language or macrolanguage of the source of a geographic name.
Description: | A macrolanguage is a set of closely related language varieties (dialects) that generally have a common linguistic identity and a common written form; this may occur when there is a transitional socio-linguistic situation in which sub-communities of a single language community are diverging. The language of the geographic name source should be distinguished from the language of origin or etymology of a geographic name; for example, considering the place name 'San Jose, California' the language of the source of this geographic name may be English if it is determined from a United States map, regardless of the fact that this geographic name means 'St. Joseph, California' in Spanish.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.languageDialectCode
Title: | ISDES.LAD
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language dialect, if applicable, of the source of a geographic name.
Description: | Some languages have no (child) dialects. Each language dialect is unique to only one parent language.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.multipleOfficialNames
Title: | ISDES.MON
Definition: | An indication that a feature has more than one official, native script, geographic name.
Description: | Multiple official names may exist when a feature passes through more than one country and those multiple countries have different official names for that feature. Some countries have more than one official language and therefore may have an official name for a feature in each official language.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | isDesignatedBy.nameIdentifier
Title: | ISDES.NFN
Definition: | The unique name identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Named Feature Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.namedFeatureIdentifier
Title: | ISDES.NFI
Definition: | The unique named feature identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Name Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullName
Title: | ISDES_2.FNA
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullNameNoDiacritics
Title: | ISDES_2.FN1
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart except that any diacritics and special characters have been replaced with their corresponding Roman characters.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullNameOrdered
Title: | ISDES_2.FN2
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart, except that its components have been arranged into an order that facilitates alphabetic ordering and search.
Description: | The component order is such that the specific part of the name appears first, followed by an optional comma, the generic part of the name, and then finally any articles or prepositions (for example: 'Everest, Mount' or 'Mexico, Gulf of'). For some geographic names no reordering of the full name is required (for example: 'Tigrus River'). Geographic names that are believed to no longer exist are enclosed in double parenthesis, as: '(( Name ))'.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.geoNameCharacterSet
Title: | ISDES_2.GCS
Definition: | The character set used for the display of characters with diacritics and special characters in a geographic name.
Description: | Individual character sets include diacritics and special characters from multiple languages in the same geographic region.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geoNameCharacterSet (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
region1 | 1 Includes language-specific characters used in the Americas and Western Europe.
region2 | 2 Includes language-specific characters used in Eastern Europe.
region3 | 3 Includes language-specific characters used in Africa and the Middle East.
region4 | 4 Includes language-specific characters used in Russia and Central Asia.
region5 | 5 Includes language-specific characters used in the Asia Pacific region.
region6 | 6 Includes language-specific characters used in Vietnam.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy_2.geoNameDesignation
Title: | ISDES_2.GND
Definition: | The designation of the type of a feature with which a geographic name is associated, as used in the NGA Geographic Names Data Base (GNDB).
Description: | A designated feature type also has a (unique, single) geographic name classification.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.geographicNameType
Title: | ISDES_2.GNT
Definition: | The type of a geographic name based on its scope of use, quality of source and/or its transliteration status.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geographicNameType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
conventional | 1 An English name that is in widespread usage for a feature that is located in a region where English is not the official language.
historicalOriginal | 9 A historical name for a feature that remains in the original (non-Latin/Roman) script.
historicalTransliterated | 8 A historical name for a feature that has been transliterated to the Latin/Roman script as necessary.
nativeOriginal | 5 The official local name for a feature that remains in the original (non-Latin/Roman) script and is approved by the U.S. Board on Geographic Names (BGN).
nativeTransliterated | 2 The official local name for a feature that has been transliterated to the Latin/Roman script as necessary and is approved by the U.S. Board on Geographic Names (BGN).
provisional | 10 A provisional name for a feature that has been transliterated to the Latin/Roman script as necessary.
unverifiedOriginal | 7 A local name for a feature that remains in the original (non-Latin/Roman) script, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
unverifiedTransliterated | 4 A local name for a feature that has been transliterated to the Latin/Roman script as necessary, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
variantOriginal | 6 A variant or alternate name for a feature that remains in the original (non-Latin/Roman) script. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
variantTransliterated | 3 A variant or alternate name for a feature that has been transliterated to the Latin/Roman script as necessary. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy_2.iso15924ScriptCode
Title: | ISDES_2.IS1
Definition: | The International Organization for Standardization (ISO 15924) four character code that designates a script.
Description: | A script is a set of graphic characters used for the written form of one or more languages.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.languageCode
Title: | ISDES_2.LAN
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language or macrolanguage of the source of a geographic name.
Description: | A macrolanguage is a set of closely related language varieties (dialects) that generally have a common linguistic identity and a common written form; this may occur when there is a transitional socio-linguistic situation in which sub-communities of a single language community are diverging. The language of the geographic name source should be distinguished from the language of origin or etymology of a geographic name; for example, considering the place name 'San Jose, California' the language of the source of this geographic name may be English if it is determined from a United States map, regardless of the fact that this geographic name means 'St. Joseph, California' in Spanish.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.languageDialectCode
Title: | ISDES_2.LAD
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language dialect, if applicable, of the source of a geographic name.
Description: | Some languages have no (child) dialects. Each language dialect is unique to only one parent language.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.multipleOfficialNames
Title: | ISDES_2.MON
Definition: | An indication that a feature has more than one official, native script, geographic name.
Description: | Multiple official names may exist when a feature passes through more than one country and those multiple countries have different official names for that feature. Some countries have more than one official language and therefore may have an official name for a feature in each official language.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | isDesignatedBy_2.nameIdentifier
Title: | ISDES_2.NFN
Definition: | The unique name identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Named Feature Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.namedFeatureIdentifier
Title: | ISDES_2.NFI
Definition: | The unique named feature identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Name Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | metadata.dataQualityStatement
Title: | MD0.DQS
Definition: | A narrative or other textual description that records a general assessment of the quality of a resource (for example: a data instance, a data set or a data processing activity).
Description: | The quality of a data resource is dependent on the data providers knowledge regarding the lineage of the data and the processes that have been used to transform that data. No restriction is placed on the length of the statement.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | metadata.delineationKnown
Title: | MD0.COD
Definition: | An indication that the delineation (for example: limits and information) of a feature is known.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | metadata.existenceCertaintyCat
Title: | MD0.COE
Definition: | A general evaluation of the quality of a feature assessment, as a category.
Multiplicity: | 0..1
Value type: | FeatureMetadata_existenceCertaintyCat (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
definite | 1 A feature whose existence has been confirmed by a trusted source.
doubtful | 2 A feature whose existence has been reported and was not able to be confirmed, but which is assumed to be present for reasons of safety.
reported | 3 A feature whose existence has been reported but not confirmed.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | metadata.surveyCoverageCategory
Title: | MD0.SUR
Definition: | A general evaluation of the coverage quality of a survey, as a category.
Description: | See possibly accompanying Attribute: 'Position Quality Category' for additional survey-related information.
Multiplicity: | 0..1
Value type: | FeatureMetadata_surveyCoverageCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
inadequatelySurveyed | 2 Surveyed, but not with complete coverage and/or not to established standards.
surveyed | 1 Surveyed with complete coverage and to established standards. Survey implies a regular, controlled survey of any date.
unsurveyed | 3 Survey data either does not exist or is very poor in coverage and/or quality.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | movementAreaEntryClearance
Title: | ENT
Definition: | The maximum entry width of a movement area considering the taxiway width plus clearance from hazards (for example: trees, revetments, and buildings).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | pavementInfo.aeroMoveAreaSurfaceCat
Title: | pavementInfo.ASX
Definition: | The level of preparation of the aerodrome movement area surface, as a category.
Description: | Common category types may range from natural to completely paved.
Multiplicity: | 0..1
Value type: | AerodromePavementInfo_aeroMoveAreaSurfaceCat (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
completelyPaved | 1 The subgrade has been prepared for load-bearing and the surface has been paved using durable materials. Intended to be a permanent surface that is highly resistant to the effects of weathering and traffic.
mostlyPaved | 2 The surface is paved for at least 50 percent of its length.
unprepared | 3 The naturally occurring surface is used without any preparation. For example: no grading or rolling.
partiallyPaved | 4 The surface is paved, but for less than 50 percent of its length.
unpaved | 5 The surface has been prepared (for example: by grading or rolling) but has not been paved. Generally considered to be only temporary in nature as unless regularly maintained the surface relatively rapidly degrades as a result of weathering and traffic. Non-local materials (for example: gravel or landing mats) may be used to improve the load-bearing and wear characteristics of the surface.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | pavementInfo.aeroMoveAreaSurfacePrep
Title: | pavementInfo.ASP
Definition: | The preparation technique(s) applied to a surface composition.
Multiplicity: | 0..1
Value type: | AerodromePavementInfo_aeroMoveAreaSurfacePrep (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
aggregateSealCoat | 1 The paved surface is seal coated to bring aggregate particles into contact with vehicle tires to improve skid resistance.
graded | 2 The movement area has been leveled to result in a smooth surface. May include a slight grade to promote drainage.
grass | 3 The surface is covered with grass.
grooved | 4 The paved surface is grooved to promote drainage and traction. Accomplished by, for example, cutting or the emplacement of plastic strips that are later removed.
oiled | 5 The surface is coated with a light layer of oil to reduce dust formation. Usually accomplished by spraying.
porousFrictionCourse | 6 The paved surface is covered by a material designed to improve drainage and reduce slippage. For example, Porous European Mix (PEM), a porous asphaltic concrete formulated with 20-24 percent air voids used as an open graded friction course (OGFC).
rolled | 7 The surface is prepared with heavy rollers to result in a firm, packed surface without local dips or swales.
rubberizedSealCoat | 8 The paved surface is seal coated using an asphalt-rubber binder. Sometimes termed a 'stress-absorbing membrane' (SAM). May be based on the use of recycled scrap tire rubber.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | pavementInfo.aeroMoveAreaSurfacePrep_2
Title: | pavementInfo.ASP_2
Definition: | The preparation technique(s) applied to a surface composition.
Multiplicity: | 0..1
Value type: | AerodromePavementInfo_aeroMoveAreaSurfacePrep (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
aggregateSealCoat | 1 The paved surface is seal coated to bring aggregate particles into contact with vehicle tires to improve skid resistance.
graded | 2 The movement area has been leveled to result in a smooth surface. May include a slight grade to promote drainage.
grass | 3 The surface is covered with grass.
grooved | 4 The paved surface is grooved to promote drainage and traction. Accomplished by, for example, cutting or the emplacement of plastic strips that are later removed.
oiled | 5 The surface is coated with a light layer of oil to reduce dust formation. Usually accomplished by spraying.
porousFrictionCourse | 6 The paved surface is covered by a material designed to improve drainage and reduce slippage. For example, Porous European Mix (PEM), a porous asphaltic concrete formulated with 20-24 percent air voids used as an open graded friction course (OGFC).
rolled | 7 The surface is prepared with heavy rollers to result in a firm, packed surface without local dips or swales.
rubberizedSealCoat | 8 The paved surface is seal coated using an asphalt-rubber binder. Sometimes termed a 'stress-absorbing membrane' (SAM). May be based on the use of recycled scrap tire rubber.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | pavementInfo.aeroMoveAreaSurfacePrep_3
Title: | pavementInfo.ASP_3
Definition: | The preparation technique(s) applied to a surface composition.
Multiplicity: | 0..1
Value type: | AerodromePavementInfo_aeroMoveAreaSurfacePrep (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
aggregateSealCoat | 1 The paved surface is seal coated to bring aggregate particles into contact with vehicle tires to improve skid resistance.
graded | 2 The movement area has been leveled to result in a smooth surface. May include a slight grade to promote drainage.
grass | 3 The surface is covered with grass.
grooved | 4 The paved surface is grooved to promote drainage and traction. Accomplished by, for example, cutting or the emplacement of plastic strips that are later removed.
oiled | 5 The surface is coated with a light layer of oil to reduce dust formation. Usually accomplished by spraying.
porousFrictionCourse | 6 The paved surface is covered by a material designed to improve drainage and reduce slippage. For example, Porous European Mix (PEM), a porous asphaltic concrete formulated with 20-24 percent air voids used as an open graded friction course (OGFC).
rolled | 7 The surface is prepared with heavy rollers to result in a firm, packed surface without local dips or swales.
rubberizedSealCoat | 8 The paved surface is seal coated using an asphalt-rubber binder. Sometimes termed a 'stress-absorbing membrane' (SAM). May be based on the use of recycled scrap tire rubber.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | pavementInfo.aeroPavementFuncStatus
Title: | pavementInfo.SFS
Definition: | The functional status of the pavement of an aerodrome movement area.
Description: | An aerodrome movement area is that part of an aerodrome to be used for aircraft movement operations, consisting of the manoeuvring area and the apron(s).
Multiplicity: | 0..1
Value type: | AerodromePavementInfo_aeroPavementFuncStatus (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
fair | 1 The condition is adequate for limited aircraft operations. It is capable of supporting 30 days of limited operations by the heaviest (highest Load Classification Number (LCN) or Aircraft Classification Number (ACN)) aircraft that can use the facility.
fairEstimated | 2 It is estimated (in lieu of reported information) that the condition is adequate for limited aircraft operations. It is estimated to be capable of supporting 30 days of limited operations by the heaviest (highest Load Classification Number (LCN) or Aircraft Classification Number (ACN)) aircraft that can use the facility.
good | 3 The condition is adequate for sustained aircraft operations. It will support 30 days of sustained operations by the heaviest (highest Load Classification Number (LCN) or Aircraft Classification Number (ACN)) aircraft that can use the facility.
goodEstimated | 4 It is estimated (in lieu of reported information) that the condition is adequate for sustained aircraft operations. It is estimated that it will support 30 days of sustained operations by the heaviest (highest Load Classification Number (LCN) or Aircraft Classification Number (ACN)) aircraft that can use the facility.
poor | 5 The condition is sufficient for only emergency aircraft operations. It will support only emergency or occasional operations by the heaviest (highest Load Classification Number (LCN) or Aircraft Classification Number (ACN)) aircraft that can use the facility.
poorEstimated | 6 It is estimated (in lieu of reported information) that the condition is sufficient for only emergency aircraft operations. It is estimated that it will support only emergency or occasional operations by the heaviest (highest Load Classification Number (LCN) or Aircraft Classification Number (ACN)) aircraft that can use the facility.
underConstruction | 7 The surface is under construction and is therefore not capable of supporting aircraft operations.
unserviceable | 8 The surface is in such a state of deterioration or disrepair that it is completely unusable and cannot be safely used for any type of aircraft operations.
excellent | 9 The surface is capable of supporting extended aircraft operations with minimal maintenance. The surface is newly constructed, less than 5 years old, and is capable of supporting extended aircraft operations by the heaviest (highest Load Classification Number (LCN) or Aircraft Classification Number (ACN)) aircraft that is rated to use the facility, with minimal need for maintenance.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | pavementInfo.loadClassificationNumber
Title: | pavementInfo.LCX
Definition: | A value which denotes the peak being moment the surface can handle repeatedly without shortening its service life.
Description: | Based on the United States Air Force/DoD LCN/LCG System.
Multiplicity: | 0..1
Value type: | Integer
## Attribute: back to top
Name: | pavementInfo.pavementClassNumber
Title: | pavementInfo.PCN
Definition: | The bearing strength of a pavement for unrestricted operations.
Multiplicity: | 0..1
Value type: | Integer
## Attribute: back to top
Name: | pavementInfo.pavementTypeForPcnDeterm
Title: | pavementInfo.PC1
Definition: | The pavement behavior (for example: rigid or flexible) used for the Pavement Classification Number (PCN) determination, as a category.
Multiplicity: | 0..1
Value type: | AerodromePavementInfo_pavementTypeForPcnDeterm (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
flexiblePavement | 1 The total pavement structure deflects, or flexes, under loading.
rigidPavement | 2 The pavement structure deflects very little under loading due to the high modulus of elasticity of the surface course.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | pavementInfo.pcnEvaluationMethod
Title: | pavementInfo.PC4
Definition: | The method used to rate a runway pavement.
Multiplicity: | 0..1
Value type: | AerodromePavementInfo_pcnEvaluationMethod (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
technical | 1 Representing a specific study of the pavement characteristics and application of pavement behaviour technology.
usingAircraftExperience | 2 Representing a knowledge of the specific type and mass of aircraft satisfactorily being supported under regular use.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | pavementInfo.pcnMaxAllowTirePressCat
Title: | pavementInfo.PC3
Definition: | The maximum allowable tire pressure category related to the Pavement Classification Number (PCN), as a category.
Multiplicity: | 0..1
Value type: | AerodromePavementInfo_pcnMaxAllowTirePressCat (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
high | 1 No pressure limit.
medium | 2 Pressure limited to 1.50 megapascal (MPa) (217 psi).
low | 3 Pressure limited to 1.00 megapascal (MPa) (145 psi).
veryLow | 4 Pressure limited to 0.50 megapascal (MPa) (73 psi).
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | pavementInfo.pcnPavementSubStrengthCat
Title: | pavementInfo.PC2
Definition: | An categorized indication of the pavement subgrade strength related to the Pavement Classification Number (PCN).
Description: | The pavement subgrade is the native material underneath a constructed pavement.
Multiplicity: | 0..1
Value type: | AerodromePavementInfo_pcnPavementSubStrengthCat (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
highStrengthSubgrade | 1 Characterized by K = 150 MN/m3 and representing all K values above 120 MN/m3 for rigid pavements, and by California Bearing Ratio (CBR) = 15 and representing all CBR values above 13 for flexible pavements.
mediumStrengthSubgrade | 2 Characterized by K = 80 MN/m3 and representing a range in K of 60 to 120 MN/m3 for rigid pavements, and by California Bearing Ratio (CBR) = 10 and representing a range in CBR of 8 to 13 for flexible pavements.
lowStrengthSubgrade | 3 Characterized by K = 40 MN/m3 and representing a range in K of 25 to 60 MN/m3 for rigid pavements, and by California Bearing Ratio (CBR) = 6 and representing a range in CBR of 4 to 8 for flexible pavements.
ultraLowStrengthSubgrade | 4 Characterized by K = 20 MN/m3 and representing all K values below 25 MN/m3 for rigid pavements, and by California Bearing Ratio (CBR) = 3 and representing all CBR values below 4 for flexible pavements.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | pavementInfo.runwayObservedLoading
Title: | pavementInfo.MDU
Definition: | A description of the heaviest aircraft observed utilizing a runway.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | permanent
Title: | PRM
Definition: | An indication that a feature is permanent.
Description: | Temporary features last, or are meant to last, for a limited time only.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | physicalCondition
Title: | PCF
Definition: | The physical condition of a man-made structure, as a whole, including the inside and/or outside of the structure and any contained and/or associated equipment.
Description: | The physical condition applies to any phase of the life cycle of a man-made structure from construction to destruction. Examples of man-made structures include roads, canals, buildings, towers, aerodromes and facilities.
Multiplicity: | 0..1
Value type: | AerodromeMoveArea_physicalCondition (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
construction | 1 The man-made structure is being built or undergoing renovation or repair. Incorporates site preparations, building of new construction and the renovation or repair of existing structures.
intact | 2 The man-made structure is complete and intact. The man-made structure may or may not be in operation or use.
unmaintained | 3 The man-made structure is left in place to deteriorate. The man-made structure has been abandoned and no maintenance or repairs are being carried out. While the structure is physically intact, no signs of operation are visible.
damaged | 4 The man-made structure is damaged. Damage may be a consequence of accident, military action, or natural disaster. The damaged man-made structure can be repaired.
dismantled | 5 The man-made structure has undergone a systematic selective removal of components. Low value components and/or equipment may remain. The man-made structure cannot be repaired without a great deal of time and effort.
destroyed | 6 The man-made structure has undergone complete destruction and is in a state of total disrepair. Destruction may be a consequence of military action, natural disaster, planned demolition or a long period of no maintenance. A destroyed man-made structure can only be restored by complete reconstruction.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | runwayBearingStrength
Title: | RBS
Definition: | The runway weight bearing capacity expressed in terms of the gross weight which is allowed for continuing operations.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | runwayMidpointElevation
Title: | RME
Definition: | The runway elevation midway between its endpoints.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | specifiedDomainValues
Title: | OTH
Definition: | One or more intended attribute domain values for one or more enumeration or codelist attributes that are not currently valid members of their respective attribute ranges.
Description: | The actual attribute domain values may have been previously, or may become in the future, valid members of the attribute domain range.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | supportedByBridgeSpan
Title: | SBB
Definition: | The object is at least partially supported by, or passes across, a bridge span.
Description: | For example, an aqueduct carried across a valley by one or more bridge spans.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | uniqueEntityIdentifier
Title: | UFI
Definition: | The globally unique and persistent identifier of an entity (for example: feature or event) instance as specified by a Uniform Resource Name (URN) in accordance with the Internet Engineering Task Force (IETF) RFC2396 and RFC2141.
Description: | It is based on the Uniform Resource Identifier (URI), a compact string of characters for identifying an abstract or physical resource. The term 'Uniform Resource Name' (URN) refers to the subset of URI that are required to remain globally unique and persistent even when the resource ceases to exist or becomes unavailable. The URN is drawn from one of a set of defined namespaces, each of which has its own set name structure and assignment procedures.
Multiplicity: | 1
Value type: | CharacterString
## Attribute: back to top
Name: | universalUniqueIdentifier
Title: | UUI
Definition: | The Universal Unique Identifier (UUID) that is assigned to a feature in order to uniquely identify it for the purpose of maintaining relationships between features (relational database) and version control.
Description: | UUIDs are defined in ITU-T Rec. X.667 |||||||||||||||||||||||||||||||| ISO/IEC 9834-8.
Multiplicity: | 1
Value type: | CharacterString