# Feature type: Tree_P

## Package: Woodlands
## Title: EC005_P
## Definition: An individual woody perennial plant, typically having a single stem or trunk growing to a considerable height and bearing lateral branches at some distance from the ground.
## Description: May be distinguished by its relative isolation from other features, thus serving as a landmark.
## Type: Feature type
## Overview of characteristics:
Attributes and association roles
Name | Type | Multiplicity
--- | --- | ---
baseElevation.accuracy | Real | 0..1
baseElevation.value-singleValue | Real | 0..1
crownDiameter-singleValue | Real | 0..1
foliageType | Tree_foliageType | 0..1
geometry-pointGeometryInfo.area | Real | 0..1
geometry-pointGeometryInfo.baseElevation.accuracy | Real | 0..1
geometry-pointGeometryInfo.baseElevation.value-singleValue | Real | 0..1
geometry-pointGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.absoluteHorizAccEvalMeth | HorizPosAccuracy_absoluteHorizAccEvalMeth | 0..1
geometry-pointGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.value | Real | 0..1
geometry-pointGeometryInfo.horizCoordMetadata.horizAccuracyCategory | HorizCoordMetadata_horizAccuracyCategory | 0..1
geometry-pointGeometryInfo.length-singleValue | Real | 0..1
geometry-pointGeometryInfo.pointGeometry | GM_Point | 0..1
geometry-pointGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.absoluteVertAccEvalMeth | VertPosAccuracy_absoluteVertAccEvalMeth | 0..1
geometry-pointGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.value | Real | 0..1
geometry-pointGeometryInfo.vertCoordMetadata.elevationAccuracyCategory | VertCoordMetadata_elevationAccuracyCategory | 0..1
geometry-pointGeometryInfo.width-singleValue | Real | 0..1
heightAboveSurfaceLevel.accuracy | Real | 0..1
heightAboveSurfaceLevel.value-singleValue | Real | 0..1
highestElevation.accuracy | Real | 0..1
highestElevation.value-singleValue | Real | 0..1
isDesignatedBy.fullName | CharacterString | 0..1
isDesignatedBy.fullNameNoDiacritics | CharacterString | 0..1
isDesignatedBy.fullNameOrdered | CharacterString | 0..1
isDesignatedBy.geoNameCharacterSet | GeoNameInfo_geoNameCharacterSet | 0..1
isDesignatedBy.geoNameDesignation | CharacterString | 0..1
isDesignatedBy.geographicNameType | GeoNameInfo_geographicNameType | 0..1
isDesignatedBy.iso15924ScriptCode | CharacterString | 0..1
isDesignatedBy.languageCode | CharacterString | 0..1
isDesignatedBy.languageDialectCode | CharacterString | 0..1
isDesignatedBy.multipleOfficialNames | BooleanWithONINA | 0..1
isDesignatedBy.nameIdentifier | CharacterString | 0..1
isDesignatedBy.namedFeatureIdentifier | CharacterString | 0..1
isDesignatedBy_2.fullName | CharacterString | 0..1
isDesignatedBy_2.fullNameNoDiacritics | CharacterString | 0..1
isDesignatedBy_2.fullNameOrdered | CharacterString | 0..1
isDesignatedBy_2.geoNameCharacterSet | GeoNameInfo_geoNameCharacterSet | 0..1
isDesignatedBy_2.geoNameDesignation | CharacterString | 0..1
isDesignatedBy_2.geographicNameType | GeoNameInfo_geographicNameType | 0..1
isDesignatedBy_2.iso15924ScriptCode | CharacterString | 0..1
isDesignatedBy_2.languageCode | CharacterString | 0..1
isDesignatedBy_2.languageDialectCode | CharacterString | 0..1
isDesignatedBy_2.multipleOfficialNames | BooleanWithONINA | 0..1
isDesignatedBy_2.nameIdentifier | CharacterString | 0..1
isDesignatedBy_2.namedFeatureIdentifier | CharacterString | 0..1
isolated | BooleanWithONINA | 0..1
metadata.dataQualityStatement | CharacterString | 0..1
metadata.delineationKnown | BooleanWithONINA | 0..1
metadata.existenceCertaintyCat | FeatureMetadata_existenceCertaintyCat | 0..1
metadata.surveyCoverageCategory | FeatureMetadata_surveyCoverageCategory | 0..1
navigationLandmark | BooleanWithONINA | 0..1
radarSignificance | Tree_radarSignificance | 0..1
specifiedDomainValues | CharacterString | 0..1
stemDiameter-singleValue | Real | 0..1
uniqueEntityIdentifier | CharacterString | 1
universalUniqueIdentifier | CharacterString | 1
vegetationSpecies | Tree_vegetationSpecies | 0..1
## Attribute: back to top
Name: | baseElevation.accuracy
Title: | BEL.accuracy
Definition: | The vertical distance from a specified vertical datum to the terrain surface of or at the base of the feature.
Description: | If the feature is not supported above the surface by another feature then the base of the feature is usually located at ground or water level on the downhill/downstream side. For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). In the case of a survey marker (monument) this is usually the elevation assigned to the marker (monument).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | baseElevation.value-singleValue
Title: | BEL.value-singleValue
Definition: | The vertical distance from a specified vertical datum to the terrain surface of or at the base of the feature.
Description: | If the feature is not supported above the surface by another feature then the base of the feature is usually located at ground or water level on the downhill/downstream side. For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). In the case of a survey marker (monument) this is usually the elevation assigned to the marker (monument).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | crownDiameter-singleValue
Title: | CRD-singleValue
Definition: | The average diameter of tree crowns within a defined area.
Description: | The tree crown displays the leaves to allow capture of radiant energy for photosynthesis. Its diameter is usually measured by projecting the edges of the crown to the ground and measuring the length along one axis from edge to edge through the crown centre. Unless the crown has a regular shape, the width measured will depend on the axis selected for measurement. Two orthogonal axes are normally selected and averaged (for example: the maximum axis and the axis at 90 degrees to it); the two measurements are then averaged using an arithmetic mean (most common) or a geometric mean (for highly elliptical boles).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | foliageType
Title: | TRE
Definition: | The predominant foliage type of the vegetation.
Multiplicity: | 0..1
Value type: | Tree_foliageType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
deciduous | 1 Sheds its leaves each year at the end of the period of growth.
evergreen | 2 Having green foliage all the year round.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | geometry-pointGeometryInfo.area
Title: | GEM-zI007.ARA
Definition: | The area within the delineation of the feature.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-pointGeometryInfo.baseElevation.accuracy
Title: | GEM-zI007.BEL.accuracy
Definition: | The vertical distance from a specified vertical datum to the terrain surface of or at the base of the feature.
Description: | If the feature is not supported above the surface by another feature then the base of the feature is usually located at ground or water level on the downhill/downstream side. For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). In the case of a survey marker (monument) this is usually the elevation assigned to the marker (monument).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-pointGeometryInfo.baseElevation.value-singleValue
Title: | GEM-zI007.BEL.value-singleValue
Definition: | The vertical distance from a specified vertical datum to the terrain surface of or at the base of the feature.
Description: | If the feature is not supported above the surface by another feature then the base of the feature is usually located at ground or water level on the downhill/downstream side. For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). In the case of a survey marker (monument) this is usually the elevation assigned to the marker (monument).
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-pointGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.absoluteHorizAccEvalMeth
Title: | GEM-zI007.horizCoordMetadata.AHA.absoluteHorizAccEvalMeth
Definition: | The method by which the absolute horizontal accuracy was derived.
Multiplicity: | 0..1
Value type: | HorizPosAccuracy_absoluteHorizAccEvalMeth (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
evaluationDeferred | 21 Evaluation deferred (no measurement).
geodeticSurveyAdequate | 1 Geodetic survey control - adequate sample.
geodeticSurveySmall | 2 Geodetic survey control - small sample.
photogrammAdequate | 22 Photogrammetric control - adequate sample.
photogrammSmall | 23 Photogrammetric control - small sample.
productSpecification | 15 Product specification accuracy value - assumed adequate sample.
sourceAccuracy | 13 Accuracy evaluation printed on the map sheet or the evaluation was derived from source accuracy.
## Attribute: back to top
Name: | geometry-pointGeometryInfo.horizCoordMetadata.absoluteHorizAccuracy90.value
Title: | GEM-zI007.horizCoordMetadata.AHA.value
Definition: | The difference between the recorded horizontal coordinates of a feature and its true position referenced to the same geodetic datum expressed as a circular error at 90 percent probability.
Description: | It may also be applied to a data set. If the data contains multiple accuracies, usually the worst accuracy which applies to 10% or more of the data is recorded.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-pointGeometryInfo.horizCoordMetadata.horizAccuracyCategory
Title: | GEM-zI007.horizCoordMetadata.ACC
Definition: | A general evaluation of the horizontal accuracy of the geographic position of a feature, as a category.
Multiplicity: | 0..1
Value type: | HorizCoordMetadata_horizAccuracyCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
accurate | 1 Meets specified accuracy requirements.
approximate | 2 Fails to meet specified accuracy requirements but is deemed sufficiently accurate for some uses.
doubtful | 3 Fails to meet specified accuracy requirements and is probably not sufficiently accurate for most uses.
precise | 7 Exceeds specified accuracy requirements.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | geometry-pointGeometryInfo.length-singleValue
Title: | GEM-zI007.LZN-singleValue
Definition: | The dimension of a feature taken along its primary alignment of use and generally in the horizontal plane.
Description: | The primary alignment of a feature is its established direction of flow or use (for example: a road, a power line, a river, a rapid, and/or a bridge). A feature-specific rule may apply. In the case of a bridge, the length is the distance between the bridge abutments along the bridge centreline. In the case of a dam, the length is the distance along the dam crest. If no established direction of flow or use exists then (1) if the feature is irregular in shape its length is its greatest horizontal dimension (see Attribute: 'Greatest Horizontal Extent'), else (2) if the feature is regular in shape then a shape-specific rule may apply: for a rectangular feature, the length of the longer axis; for a round feature, the diameter.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-pointGeometryInfo.pointGeometry
Title: | GEM-zI007.G01
Definition: | A 0-dimensional geometric primitive, representing a position.
Multiplicity: | 0..1
Value type: | GM_Point
## Attribute: back to top
Name: | geometry-pointGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.absoluteVertAccEvalMeth
Title: | GEM-zI007.vertCoordMetadata.AVA.absoluteVertAccEvalMeth
Definition: | The method by which the absolute vertical accuracy was derived.
Multiplicity: | 0..1
Value type: | VertPosAccuracy_absoluteVertAccEvalMeth (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
evaluationDeferred | 21 Evaluation deferred (no measurement).
geodeticSurveyAdequate | 1 Geodetic survey control - adequate sample.
geodeticSurveySmall | 2 Geodetic survey control - small sample.
photogrammAdequate | 22 Photogrammetric control - adequate sample.
photogrammSmall | 23 Photogrammetric control - small sample.
productSpecification | 15 Product specification accuracy value - assumed adequate sample.
sourceAccuracy | 13 Accuracy evaluation printed on the map sheet or the evaluation was derived from source accuracy.
## Attribute: back to top
Name: | geometry-pointGeometryInfo.vertCoordMetadata.absoluteVertAccuracy90.value
Title: | GEM-zI007.vertCoordMetadata.AVA.value
Definition: | The difference between the recorded elevation of a feature and its true elevation referenced to the same vertical datum expressed as a linear error at 90 percent probability.
Description: | It may also be applied to a data set. If the data contains multiple accuracies, usually the worst accuracy which applies to 10% or more of the data is recorded.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | geometry-pointGeometryInfo.vertCoordMetadata.elevationAccuracyCategory
Title: | GEM-zI007.vertCoordMetadata.ELA
Definition: | A general evaluation of the accuracy of the vertical position of a feature, as a category.
Multiplicity: | 0..1
Value type: | VertCoordMetadata_elevationAccuracyCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
accurate | 1 Meets specified accuracy requirements.
approximate | 2 Fails to meet specified accuracy requirements but is deemed sufficiently accurate for some uses.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | geometry-pointGeometryInfo.width-singleValue
Title: | GEM-zI007.WID-singleValue
Definition: | The dimension of a feature taken perpendicular to its primary alignment of use and generally in the horizontal plane.
Description: | The primary alignment of a feature is its established direction of flow or use (for example: a road, a power line right-of-way, a river, rapid, and/or a bridge). A feature-specific rule may apply. In the case of a bridge, the width is the distance perpendicular to the bridge centre-line and generally in the horizontal plane. In the case of a dam, the width is the distance perpendicular to (across the) the dam crest. If no such direction of flow or use exists then (1) if the feature is irregular in shape its width is taken perpendicular to the direction of its greatest horizontal dimension (see Attribute: 'Greatest Horizontal Extent'), else (2) if the feature is regular in shape then a shape-specific rule may apply: for a rectangular feature, the length of the shorter axis; for a round feature, the diameter.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | heightAboveSurfaceLevel.accuracy
Title: | HGT.accuracy
Definition: | The vertical distance measured from the lowest point of the base of the feature at ground or water level (downhill/downstream side) to the tallest point of the feature.
Description: | For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). Note that the feature may be supported above the surface by another feature (for example: a tower supported by a building) and as a consequence the value of the Height Above Surface Level is different (larger) than the base-to-top height of the feature (for example: supported tower) itself.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | heightAboveSurfaceLevel.value-singleValue
Title: | HGT.value-singleValue
Definition: | The vertical distance measured from the lowest point of the base of the feature at ground or water level (downhill/downstream side) to the tallest point of the feature.
Description: | For non-inland water bodies, the water level is usually understood to be Mean Sea Level (MSL). Note that the feature may be supported above the surface by another feature (for example: a tower supported by a building) and as a consequence the value of the Height Above Surface Level is different (larger) than the base-to-top height of the feature (for example: supported tower) itself.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | highestElevation.accuracy
Title: | ZVH.accuracy
Definition: | The elevation from a specified vertical datum to the highest point on a feature.
Description: | In the case of multiple features that may be stacked on each other (for example: a railway on a bridge, a superstructure on a building, or an aerial on a tower) the highest elevation is that of the entire feature stack. For example, the highest elevation of a church is that of its steeple and not that of the roof of the church itself. The church itself may have a height above surface level that excludes the additional height of the steeple superstructure located on the church roof.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | highestElevation.value-singleValue
Title: | ZVH.value-singleValue
Definition: | The elevation from a specified vertical datum to the highest point on a feature.
Description: | In the case of multiple features that may be stacked on each other (for example: a railway on a bridge, a superstructure on a building, or an aerial on a tower) the highest elevation is that of the entire feature stack. For example, the highest elevation of a church is that of its steeple and not that of the roof of the church itself. The church itself may have a height above surface level that excludes the additional height of the steeple superstructure located on the church roof.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | isDesignatedBy.fullName
Title: | ISDES.FNA
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.fullNameNoDiacritics
Title: | ISDES.FN1
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart except that any diacritics and special characters have been replaced with their corresponding Roman characters.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.fullNameOrdered
Title: | ISDES.FN2
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart, except that its components have been arranged into an order that facilitates alphabetic ordering and search.
Description: | The component order is such that the specific part of the name appears first, followed by an optional comma, the generic part of the name, and then finally any articles or prepositions (for example: 'Everest, Mount' or 'Mexico, Gulf of'). For some geographic names no reordering of the full name is required (for example: 'Tigrus River'). Geographic names that are believed to no longer exist are enclosed in double parenthesis, as: '(( Name ))'.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.geoNameCharacterSet
Title: | ISDES.GCS
Definition: | The character set used for the display of characters with diacritics and special characters in a geographic name.
Description: | Individual character sets include diacritics and special characters from multiple languages in the same geographic region.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geoNameCharacterSet (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
region1 | 1 Includes language-specific characters used in the Americas and Western Europe.
region2 | 2 Includes language-specific characters used in Eastern Europe.
region3 | 3 Includes language-specific characters used in Africa and the Middle East.
region4 | 4 Includes language-specific characters used in Russia and Central Asia.
region5 | 5 Includes language-specific characters used in the Asia Pacific region.
region6 | 6 Includes language-specific characters used in Vietnam.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy.geoNameDesignation
Title: | ISDES.GND
Definition: | The designation of the type of a feature with which a geographic name is associated, as used in the NGA Geographic Names Data Base (GNDB).
Description: | A designated feature type also has a (unique, single) geographic name classification.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.geographicNameType
Title: | ISDES.GNT
Definition: | The type of a geographic name based on its scope of use, quality of source and/or its transliteration status.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geographicNameType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
conventional | 1 An English name that is in widespread usage for a feature that is located in a region where English is not the official language.
historicalOriginal | 9 A historical name for a feature that remains in the original (non-Latin/Roman) script.
historicalTransliterated | 8 A historical name for a feature that has been transliterated to the Latin/Roman script as necessary.
nativeOriginal | 5 The official local name for a feature that remains in the original (non-Latin/Roman) script and is approved by the U.S. Board on Geographic Names (BGN).
nativeTransliterated | 2 The official local name for a feature that has been transliterated to the Latin/Roman script as necessary and is approved by the U.S. Board on Geographic Names (BGN).
provisional | 10 A provisional name for a feature that has been transliterated to the Latin/Roman script as necessary.
unverifiedOriginal | 7 A local name for a feature that remains in the original (non-Latin/Roman) script, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
unverifiedTransliterated | 4 A local name for a feature that has been transliterated to the Latin/Roman script as necessary, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
variantOriginal | 6 A variant or alternate name for a feature that remains in the original (non-Latin/Roman) script. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
variantTransliterated | 3 A variant or alternate name for a feature that has been transliterated to the Latin/Roman script as necessary. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy.iso15924ScriptCode
Title: | ISDES.IS1
Definition: | The International Organization for Standardization (ISO 15924) four character code that designates a script.
Description: | A script is a set of graphic characters used for the written form of one or more languages.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.languageCode
Title: | ISDES.LAN
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language or macrolanguage of the source of a geographic name.
Description: | A macrolanguage is a set of closely related language varieties (dialects) that generally have a common linguistic identity and a common written form; this may occur when there is a transitional socio-linguistic situation in which sub-communities of a single language community are diverging. The language of the geographic name source should be distinguished from the language of origin or etymology of a geographic name; for example, considering the place name 'San Jose, California' the language of the source of this geographic name may be English if it is determined from a United States map, regardless of the fact that this geographic name means 'St. Joseph, California' in Spanish.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.languageDialectCode
Title: | ISDES.LAD
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language dialect, if applicable, of the source of a geographic name.
Description: | Some languages have no (child) dialects. Each language dialect is unique to only one parent language.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.multipleOfficialNames
Title: | ISDES.MON
Definition: | An indication that a feature has more than one official, native script, geographic name.
Description: | Multiple official names may exist when a feature passes through more than one country and those multiple countries have different official names for that feature. Some countries have more than one official language and therefore may have an official name for a feature in each official language.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | isDesignatedBy.nameIdentifier
Title: | ISDES.NFN
Definition: | The unique name identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Named Feature Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy.namedFeatureIdentifier
Title: | ISDES.NFI
Definition: | The unique named feature identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Name Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullName
Title: | ISDES_2.FNA
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullNameNoDiacritics
Title: | ISDES_2.FN1
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart except that any diacritics and special characters have been replaced with their corresponding Roman characters.
Description: | It is generally considered to consist of a specific part, a generic part, and any articles or prepositions. The order of the parts may vary with the generic part appearing at the beginning, middle or end.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.fullNameOrdered
Title: | ISDES_2.FN2
Definition: | A complete name that is used to designate the entity as that designation would normally be written by the originating culture on a map or chart, except that its components have been arranged into an order that facilitates alphabetic ordering and search.
Description: | The component order is such that the specific part of the name appears first, followed by an optional comma, the generic part of the name, and then finally any articles or prepositions (for example: 'Everest, Mount' or 'Mexico, Gulf of'). For some geographic names no reordering of the full name is required (for example: 'Tigrus River'). Geographic names that are believed to no longer exist are enclosed in double parenthesis, as: '(( Name ))'.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.geoNameCharacterSet
Title: | ISDES_2.GCS
Definition: | The character set used for the display of characters with diacritics and special characters in a geographic name.
Description: | Individual character sets include diacritics and special characters from multiple languages in the same geographic region.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geoNameCharacterSet (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
region1 | 1 Includes language-specific characters used in the Americas and Western Europe.
region2 | 2 Includes language-specific characters used in Eastern Europe.
region3 | 3 Includes language-specific characters used in Africa and the Middle East.
region4 | 4 Includes language-specific characters used in Russia and Central Asia.
region5 | 5 Includes language-specific characters used in the Asia Pacific region.
region6 | 6 Includes language-specific characters used in Vietnam.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy_2.geoNameDesignation
Title: | ISDES_2.GND
Definition: | The designation of the type of a feature with which a geographic name is associated, as used in the NGA Geographic Names Data Base (GNDB).
Description: | A designated feature type also has a (unique, single) geographic name classification.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.geographicNameType
Title: | ISDES_2.GNT
Definition: | The type of a geographic name based on its scope of use, quality of source and/or its transliteration status.
Multiplicity: | 0..1
Value type: | GeoNameInfo_geographicNameType (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
conventional | 1 An English name that is in widespread usage for a feature that is located in a region where English is not the official language.
historicalOriginal | 9 A historical name for a feature that remains in the original (non-Latin/Roman) script.
historicalTransliterated | 8 A historical name for a feature that has been transliterated to the Latin/Roman script as necessary.
nativeOriginal | 5 The official local name for a feature that remains in the original (non-Latin/Roman) script and is approved by the U.S. Board on Geographic Names (BGN).
nativeTransliterated | 2 The official local name for a feature that has been transliterated to the Latin/Roman script as necessary and is approved by the U.S. Board on Geographic Names (BGN).
provisional | 10 A provisional name for a feature that has been transliterated to the Latin/Roman script as necessary.
unverifiedOriginal | 7 A local name for a feature that remains in the original (non-Latin/Roman) script, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
unverifiedTransliterated | 4 A local name for a feature that has been transliterated to the Latin/Roman script as necessary, where a native source for the name was either unavailable or nonexistant and a non-native source for the name was used instead and the resulting name could not be verified from a recent local official source. An unverified name is usually indicated in a gazetteer using the dagger symbol.
variantOriginal | 6 A variant or alternate name for a feature that remains in the original (non-Latin/Roman) script. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
variantTransliterated | 3 A variant or alternate name for a feature that has been transliterated to the Latin/Roman script as necessary. For example, a former name, a name in local usage, alternate name spellings found in various sources, or a derived short name.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | isDesignatedBy_2.iso15924ScriptCode
Title: | ISDES_2.IS1
Definition: | The International Organization for Standardization (ISO 15924) four character code that designates a script.
Description: | A script is a set of graphic characters used for the written form of one or more languages.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.languageCode
Title: | ISDES_2.LAN
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language or macrolanguage of the source of a geographic name.
Description: | A macrolanguage is a set of closely related language varieties (dialects) that generally have a common linguistic identity and a common written form; this may occur when there is a transitional socio-linguistic situation in which sub-communities of a single language community are diverging. The language of the geographic name source should be distinguished from the language of origin or etymology of a geographic name; for example, considering the place name 'San Jose, California' the language of the source of this geographic name may be English if it is determined from a United States map, regardless of the fact that this geographic name means 'St. Joseph, California' in Spanish.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.languageDialectCode
Title: | ISDES_2.LAD
Definition: | The International Organization for Standardization (ISO 639-3) three character code that designates the language dialect, if applicable, of the source of a geographic name.
Description: | Some languages have no (child) dialects. Each language dialect is unique to only one parent language.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.multipleOfficialNames
Title: | ISDES_2.MON
Definition: | An indication that a feature has more than one official, native script, geographic name.
Description: | Multiple official names may exist when a feature passes through more than one country and those multiple countries have different official names for that feature. Some countries have more than one official language and therefore may have an official name for a feature in each official language.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | isDesignatedBy_2.nameIdentifier
Title: | ISDES_2.NFN
Definition: | The unique name identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Named Feature Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isDesignatedBy_2.namedFeatureIdentifier
Title: | ISDES_2.NFI
Definition: | The unique named feature identifier element in the NGA Geographic Names Data Base (GNDB).
Description: | Typically used together with Attribute: 'Name Identifier' to provide a unique index into the NGA Geographic Names Data Base (GNDB) from which NGA draws all of its feature name information.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | isolated
Title: | ISS
Definition: | An indication that a feature (for example: a structure) is in the open by itself, isolated from other features of a similar type, and thus is visually distinct from surrounding features when viewed from a distance.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | metadata.dataQualityStatement
Title: | MD0.DQS
Definition: | A narrative or other textual description that records a general assessment of the quality of a resource (for example: a data instance, a data set or a data processing activity).
Description: | The quality of a data resource is dependent on the data providers knowledge regarding the lineage of the data and the processes that have been used to transform that data. No restriction is placed on the length of the statement.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | metadata.delineationKnown
Title: | MD0.COD
Definition: | An indication that the delineation (for example: limits and information) of a feature is known.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | metadata.existenceCertaintyCat
Title: | MD0.COE
Definition: | A general evaluation of the quality of a feature assessment, as a category.
Multiplicity: | 0..1
Value type: | FeatureMetadata_existenceCertaintyCat (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
definite | 1 A feature whose existence has been confirmed by a trusted source.
doubtful | 2 A feature whose existence has been reported and was not able to be confirmed, but which is assumed to be present for reasons of safety.
reported | 3 A feature whose existence has been reported but not confirmed.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | metadata.surveyCoverageCategory
Title: | MD0.SUR
Definition: | A general evaluation of the coverage quality of a survey, as a category.
Description: | See possibly accompanying Attribute: 'Position Quality Category' for additional survey-related information.
Multiplicity: | 0..1
Value type: | FeatureMetadata_surveyCoverageCategory (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
inadequatelySurveyed | 2 Surveyed, but not with complete coverage and/or not to established standards.
surveyed | 1 Surveyed with complete coverage and to established standards. Survey implies a regular, controlled survey of any date.
unsurveyed | 3 Survey data either does not exist or is very poor in coverage and/or quality.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | navigationLandmark
Title: | LMC
Definition: | An indication that a feature may serve as a navigation landmark, allowing for rapid and positive orientation of a navigator.
Description: | Its size, shape, and/or location make it prominent in relation to its surroundings, and it is therefore easily recognized from the surface and/or from the air.
Multiplicity: | 0..1
Value type: | BooleanWithONINA (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
false | 1000 False
true | 1001 True
noInformation | -999999 No Information
## Attribute: back to top
Name: | radarSignificance
Title: | RSI
Definition: | The predominant exposed surface material, categorized by its significance to radar-based sensors.
Multiplicity: | 0..1
Value type: | Tree_radarSignificance (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
metal | 1 75 percent or greater of the surface is metal (for example: tin, steel, corrugated iron, or aluminum). For example, aluminum mobile homes, steel storage tanks, steel bridge super/substructures, or steel power transmission line pylons. For built-up areas the surface considered includes the roof area but excludes the ground and ground-level pavements.
partMetal | 2 40 to 74 percent of the surface is metal with any remaining surface being some other material (for example: wood, stone, brick, or concrete). For example, railway or metal ore slag dumps. For built-up areas the surface considered includes the roof area but excludes the ground and ground-level pavements.
masonry | 3 Either: 75 percent or more of the surface is stone, brick or concrete, mixed with up to 25 percent wood, glass or composition; or 50 to 75 percent of the surface is stone, brick and/or concrete mixed with 5 to 39 percent metal surface with any remaining surface being some other material (for example: wood or plastic). For example, school buildings, commercial buildings, apartment houses, houses, walls, or cemetery buildings/tombs. For built-up areas the surface considered includes the roof area but excludes the ground and ground-level pavements.
composition | 4 Either: 50 to 74 percent of the surface is stone, brick and/or concrete mixed with 25 to 50 percent wood, plastic, glass or composition with any remaining surface being some other material (for example: slate or tar paper); 51 percent or more of the surface is composition, slate, tar paper, and/or glass with any remaining surface being some other material (for example: stone or brick)$$$$$ or 75 percent or more of the surface is wood, mixed with up to 25 percent composition, plastic, and/or glass. For example, residential housing and agricultural buildings. For built-up areas the surface considered includes the roof area but excludes the ground and ground-level pavements.
earthen | 5 51 percent or greater of the surface is land, soil, or ground surface characteristics with any remaining surface being some other material (for example: stone or brick). For example, storage bunkers for munitions, embankments, cuttings, earthen dams, levees, loose or light surface roads, mine tailings, and mineral piles. It does not include metal ore storage.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other
## Attribute: back to top
Name: | specifiedDomainValues
Title: | OTH
Definition: | One or more intended attribute domain values for one or more enumeration or codelist attributes that are not currently valid members of their respective attribute ranges.
Description: | The actual attribute domain values may have been previously, or may become in the future, valid members of the attribute domain range.
Multiplicity: | 0..1
Value type: | CharacterString
## Attribute: back to top
Name: | stemDiameter-singleValue
Title: | SDS-singleValue
Definition: | The average diameter of the tree trunks in an area, measured at a height of approximately 1.5 metres or 4.5 feet on the high side (if on a hillside) above the surface of the ground.
Description: | Commonly referred to as the 'diameter at breast height' (dbh). For trees up to 2 metres high, the stem diameter is measured at the mid-point between the ground and the stem tip.
Multiplicity: | 0..1
Value type: | Real
## Attribute: back to top
Name: | uniqueEntityIdentifier
Title: | UFI
Definition: | The globally unique and persistent identifier of an entity (for example: feature or event) instance as specified by a Uniform Resource Name (URN) in accordance with the Internet Engineering Task Force (IETF) RFC2396 and RFC2141.
Description: | It is based on the Uniform Resource Identifier (URI), a compact string of characters for identifying an abstract or physical resource. The term 'Uniform Resource Name' (URN) refers to the subset of URI that are required to remain globally unique and persistent even when the resource ceases to exist or becomes unavailable. The URN is drawn from one of a set of defined namespaces, each of which has its own set name structure and assignment procedures.
Multiplicity: | 1
Value type: | CharacterString
## Attribute: back to top
Name: | universalUniqueIdentifier
Title: | UUI
Definition: | The Universal Unique Identifier (UUID) that is assigned to a feature in order to uniquely identify it for the purpose of maintaining relationships between features (relational database) and version control.
Description: | UUIDs are defined in ITU-T Rec. X.667 |||||||||||||||||||||||||||||||| ISO/IEC 9834-8.
Multiplicity: | 1
Value type: | CharacterString
## Attribute: back to top
Name: | vegetationSpecies
Title: | VSP
Definition: | The predominant species of a tract of vegetation.
Multiplicity: | 0..1
Value type: | Tree_vegetationSpecies (enumeration)
Values: | See listed values
Value Name | Documentation
--- | ---
alder | 40 A member of the birch family that grows in moist places (Alnus glutinosa). The light wood is known for being extremely durable under water.
ash | 1 A forest tree, Fraxinus excelsior, with grey bark, pinnate foliage, and hard, tough, pale wood. Also (with specifying word), any of various related or otherwise similar trees; especially any other tree of the genus Fraxinus.
aspen | 41 The trembling poplar (Populus tremula). Remarkable for its quivering leaves.
baobab | 37 An African tree (Adansonia digitata) with a short thick stem and a broad crown. It is capable of storing great quantities of water.
beech | 2 A forest tree of the genus Fagus, having thin, smooth bark and glossy oval leaves, and bearing nuts. Especially the European Fagus sylvatica. Also (usually with specifying word), any of various similar trees, especially (in the southern hemisphere) of the genus Nothofagus.
birch | 3 Any of various hardy northern trees or shrubs of the genus Betula (family Betulaceae), having smooth, tough bark and slender branches. Especially (in Europe) Betula pendula (more fully silver birch) and Betula pubescens (more fully downy birch), and (in North America) Betula papyrifera (more fully paper birch).
casuarina | 4 A tree of the genus Casuarina (family Casuarinaceae) with jointed branches resembling gigantic horsetail plants. It is native to Australia and parts of Southeast Asia.
cedar | 54 An evergreen coniferous tree, such as Abies cedrus. It has durable and fragrant wood.
cembraPine | 55 An alpine coniferous genus (Pinus cembra). The wood is resinous, durable and is used for panelling and carving.
chestnut | 5 A tree of the genus Castanea, of the beech family. Especially that of Castanea sativa (also Spanish chestnut, sweet chestnut). Also (with specifying word), any of various similar trees.
coconut | 33 A tropical palm tree, Cocos nucifera, that bears a large ovate brown hard-shelled seed having an edible white lining enclosing a white liquid. Its fruitflesh (Copra) is also processed for the production of oil, fat and dried cocoflakes.
conifer | 6 A gymnospermous tree or shrub of the order Coniferales, members of which typically bear cones and evergreen needle-like leaves. For example, the pines, firs, cedars, larches, spruces, and yews.
corkOak | 7 An evergreen oak, Quercus suber, which is native to the Mediterranean and has the distinctive property of producing more cork after some is removed. Industrially used for various kinds of cork based products.
cypress | 8 An evergreen coniferous tree of the Eurasian and North American genus Cupressus having flattened shoots with scalelike leaves. For example, Cupressus sempervirens (also known as Italian cypress), a tall, often fastigiate, tree native to southern Europe and the Middle East, with dark foliage and hard durable wood.
douglasFir | 38 A coniferous timber tree of the genus Abies. Used for veneer, furniture or construction.
elm | 9 Any of various deciduous trees with serrate leaves, of the genus Ulmus and other genera of the family Ulmaceae. Especially (a) (more fully English elm) the European Ulmaceae procera, once common as a hedge tree in central and southern England; (b) (more fully American elm or white elm) Ulmaceae americana, a tree with pale bark of eastern North America.
eucalyptus | 10 Any of the genus Eucalyptus of flowering evergreen trees and shrubs, of the myrtle family. Includes species important as forest trees in Australia and grown elsewhere for their hardwood, oils, gums, and resins, and as ornamentals.
filao | 11 Casuarina equisetifolia, the most widespread and well-known member of the family Casuarinaceae. Known by many names including: Casuarina, ironwood, coast she-oak, horsetail, Australian pine, whistling pine, beefwood, agoho (Philippines), ru (Malaysia), filao (Vietnam, West Africa, West Indies) and nokonoko (Fiji).
fir | 12 An evergreen coniferous tree, especially one belonging to the genus Abies of the pine family, characterized by upright cones and flat needles usually arranged in two rows. Naturally occuring in the temperate zones of the northern hemisphere. Firs consist of more than fifty species.
gaboon | 48 A medium-sized hardwood tree of Western Africa (Aucoumea klaineana). Often used for furniture.
hazel | 14 Any of various deciduous shrubs and low trees constituting the genus Corylus, of the birch family, bearing edible nuts enclosed in leafy involucres. Especially the European hazel, Corylus avellana, and its North American counterpart, Corylus americana.
hickory | 43 One of several Norh American trees of the genus Carya. Related to the walnuts, especially Carya alba, the timber of which is tough and elastic.
hornbeam | 42 A small tree of the northern hemisphere (Carpinus betulus). Yields tough timber and is cultivated for planting hedges.
ilex | 16 A kind of oak, Quercus ilex, common in Mediterranean countries, with dark evergreen sometimes spiny-toothed leaves.
ilexAquifolium | 60 Ilex Aquifolium (Holly, or European Holly to distinguish it from related species) is an evergreen tree growing to 10-25 metres tall with smooth grey bark whose leaves are 5-12 centimetres long and 2-6 centimetres broad with three to five sharp spines on each side. A species of holly native to western and southern Europe, northwest Africa and southwest Asia.
juniper | 59 A genus of prickly evergreen shrubs, comprising Juniperus communis. Popular in the northern hemisphere on arid soils. Used as ornamental plant or for medicinal purposes.
larch | 18 Any of various deciduous coniferous trees of the genus Larix. Specifically Larix decidua, native to the Alps and cultivated for its tough durable timber.
laurel | 45 A glossy-leaved evergreen shrub (Laurus nobilis), popular in the Mediterranian region. The leaves are used for spice; the oil of the fruits has medicinal properties.
mahogany | 46 A tree of tropical America (Swietenia mahagoni). Yields a hard, fine-grained wood, used for building instruments and for woodwork arts.
mangrove | 19 Any of various tropical trees or shrubs of the genera Rhizophora and Bruguiera (family Rhizophoraceae) with interlacing aerial roots, which form dense thickets in muddy swamps subject to tidal inundation. For example, Rhizophora mangle (also known as common mangrove or red mangrove). May also be used to describe other tropical trees or shrubs of similar habit and appearance, especially of the genus Avicennia (of the verbena family).
maple | 20 A Eurasian tree, Acer campestre (family Aceraceae), with fruit in the form of two winged samaras joined together and palmately lobed leaves (more fully common maple, hedge maple). Also (with specifying word), any of numerous similar trees of this or other genera.
oak | 23 Any of numerous trees (rarely shrubs) of the genus Quercus, of the beech family, with acorns borne in cupules and frequently with sinuately lobed leaves. Specifically (more fully common oak, English oak, pedunculate oak) Quercus robur and (more fully durmast oak, sessile oak) Quercus petraea.
olive | 24 An evergreen tree, Olea europaea (family Oleaceae), with narrow leaves hoary on the underside and small whitish flowers. Long cultivated in the Mediterranean region for its fruit and the oil obtained from this. May also be used to describe any of various wild trees or shrubs of the genus Olea; (with specifying word) any of various trees and shrubs allied to the common olive, or resembling it in appearance or in providing oil.
osier | 57 A species of willow, Salix viminalis, growing close to waterbodies or on moist ground. The pliable shoots of it are used for basket-making.
pine | 26 Any coniferous tree of the genus Pinus, comprising usually large trees with evergreen needle-shaped leaves growing in clusters. Native to northern temperate regions, and valued especially as a source of timber, tar, and turpentine.
plane | 49 A tree having large spreading branches with broad angular leaves, one of various species of the genus Platanus. Often grown as avenue-, ornamental- and park-tree.
poplar | 27 Any of various often tall and fast-growing, sometimes narrowly erect, trees of the genus Populus, of the willow family, often with triangular-ovate leaves. May also be used to describe any of various other trees resembling the poplar: specifically (a) in North America the tulip tree, Liriodendron tulipifera; (b) in Australia either of two trees with leaves like those of many poplars, Homalanthus populifolius, of the spurge family, and (more fully native poplar) Codonocarpus cotinifolius (family Gyrostemonaceae).
posidonia | 28 Posidonia oceanica, an alga-like, vascular, flowering plant endemic to the Mediterranean Sea. It forms extensive underwater meadows that spread from the shore to the depth of 40 metres. Most often they are found on silty and sandy floors; less often on hard ground. Its rhizomes, which can grow horizontally or vertically, are densely intertwined and constitute a kind of a secondary bottom. This may be several decimetres thick and can sometimes create actual reefs.
sequoia | 47 A Californian genus of gigantic conifers. Has two species; the highest trees in the world.
spruce | 56 A coniferous of the genus Picea, popular on the northern hemisphere. Used for construction and trimmed timber.
teak | 51 A large East Indian tree (Tectona grandis). Yields a heavy timber.
thuya | 52 A genus of coniferous trees or shrubs (Thuja) of the cypress family. Often cultivated for planting hedges.
umbrellaThorn | 50 A species of acacia (Acacia tortilis). Has an umbrella like crown. The mark of Africa.
walnut | 32 Any tree of the genus Juglans (family Juglandaceae), members of which have drooping catkins and aromatic pinnate leaves. Especially the Eurasian Juglans regia and (more fully black walnut) the North American Juglans nigra. The green fleshy fruit contains an edible kernel in separate halves.
yew | 58 A darkleaved evergreen shrub or tree of the genus Taxus. All parts of the plant are poisonous.
nipa | 22 A palm tree, Nypa fruticans, of mangrove swamps in tropical Asia and Australia, having a creeping rhizome and large feathery leaves.
palm | 25 Any tree or shrub of the large, chiefly tropical, monocotyledonous family Palmae, typically having an unbranched stem with a crown of very large leaves either palmate or pinnate in shape. Also (with specifying word), any of various palmlike plants of other families, such as cycads.
bamboo | 34 Any of numerous, mainly tropical, giant grasses belonging to the genus Bambusa and various related genera. The mature canes are used for construction and furniture.
noInformation | -999999 No Information
notApplicable | 998 Not Applicable
other | 999 Other