# Package: VesselStorageRepairFacilities

Parent: PortsHarbours

## Relevant types:

Name | Type | Definition | Description
--- | --- | --- | ---
DryDock_P | Feature Type | An artificial basin fitted with a gate or caisson into which vessels can be floated and the water pumped out to expose the bottom of the vessel. | -
DryDock_S | Feature Type | An artificial basin fitted with a gate or caisson into which vessels can be floated and the water pumped out to expose the bottom of the vessel. | -
FloatingDryDock_P | Feature Type | A form of dry dock consisting of a floating structure of one or more sections which can be partly submerged by controlled flooding to receive a vessel, then raised by pumping out the water so that the vessel's bottom can be exposed. | -
FloatingDryDock_S | Feature Type | A form of dry dock consisting of a floating structure of one or more sections which can be partly submerged by controlled flooding to receive a vessel, then raised by pumping out the water so that the vessel's bottom can be exposed. | -
Gridiron_C | Feature Type | A timber structure in the intertidal zone serving as a support for vessels at low stages of the tide to permit work on the exposed portion of the vessel's hull. | -
Gridiron_P | Feature Type | A timber structure in the intertidal zone serving as a support for vessels at low stages of the tide to permit work on the exposed portion of the vessel's hull. | -
Gridiron_S | Feature Type | A timber structure in the intertidal zone serving as a support for vessels at low stages of the tide to permit work on the exposed portion of the vessel's hull. | -