# Package: CommunicationFacilities

Parent: Cultural

## Relevant types:

Name | Type | Definition | Description
--- | --- | --- | ---
AerialFarm_P | Feature Type | A collection of aerials that are collocated and serve a common purpose. | They may be organized either to function as a single larger virtual device (for example: a phased array) or function relatively independently of each other (for example: pointed in different directions and operating at different frequencies as at a satellite communication ground station).
AerialFarm_S | Feature Type | A collection of aerials that are collocated and serve a common purpose. | They may be organized either to function as a single larger virtual device (for example: a phased array) or function relatively independently of each other (for example: pointed in different directions and operating at different frequencies as at a satellite communication ground station).
Aerial_C | Feature Type | A device that is used for emitting and/or sensing electromagnetic energy. | For example, used to transmit and/or receive electronic signals as on a radio tower or to capture electromagnetic energy as in radio astronomy.
Aerial_P | Feature Type | A device that is used for emitting and/or sensing electromagnetic energy. | For example, used to transmit and/or receive electronic signals as on a radio tower or to capture electromagnetic energy as in radio astronomy.
Aerial_S | Feature Type | A device that is used for emitting and/or sensing electromagnetic energy. | For example, used to transmit and/or receive electronic signals as on a radio tower or to capture electromagnetic energy as in radio astronomy.
Cable_C | Feature Type | A single continuous rope-like bundle consisting of multiple strands. | The strands may be individually insulated and/or protected and the cable as a whole sheathed. Cables may be used for load bearing (for example, supporting or suspending equipment and/or structures), transmitting electrical power, and/or communicating signals (for example, by electrical or optical means).
DishAerial_P | Feature Type | A concave-shaped aerial that is used for emitting and/or sensing electromagnetic energy. | For example, used to transmit and/or receive electronic signals as at a satellite station or to capture electromagnetic energy as in radio astronomy.
DishAerial_S | Feature Type | A concave-shaped aerial that is used for emitting and/or sensing electromagnetic energy. | For example, used to transmit and/or receive electronic signals as at a satellite station or to capture electromagnetic energy as in radio astronomy.
Pylon_P | Feature Type | A pylon or pole used to support one or more cables. | -
Pylon_S | Feature Type | A pylon or pole used to support one or more cables. | -
Tower_P | Feature Type | A relatively tall, narrow structure that may either stand alone or may form part of another structure. | Usually of a square, circular, or rectangular cross-section.
Tower_S | Feature Type | A relatively tall, narrow structure that may either stand alone or may form part of another structure. | Usually of a square, circular, or rectangular cross-section.